SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-START_432-373
	Type ( Engine )
	WagonShape ( H-START_432-373.s )
	Name ( "H-START_432-373" )
	Size ( 4.547m 4.5m 15.373m ) 
	CentreOfGravity ( 0m 0m 0m )
	Mass ( 80t ) 
	WheelRadius ( 0.590m ) 
	InertiaTensor ( Box ( 4.547m 4.5m 15.373m ) )
	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
    CouplingHasRigidConnection ( 1 )
    Velocity ( 0.01m/s )
    )
comment ( Front Coupler )
	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
    CouplingHasRigidConnection ( 1 )
    Velocity ( 0.01m/s )
    )
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
      )
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
    )
	Adheasion ( 0.1 0.36 1 0 ) 
	DerailRailHeight ( 4cm )
	DerailRailForce ( 400*2.5t )
	DerailBufferForce ( 2000kN )
	NumWheels ( 4 )	comment ( 4 tengelyes a mozdony B'B' tengelyelrendezessel [6/107] )
	comment ( MSTS menetellenallas parameterek jelentese a dokumentacio alapjan:
			C1		E1		V2		C2		E2
		C1,C2,E1,E2 konstansok, V2 sebesseghatar m/s (elso sor) vagy rad/s-ban (masodik sor)
		V aktualis sebesseg
		Ha V=<V2, akkor Fme(MSTS)=C1*V^E1
		Ha V>V2, akkor Fme(MSTS)=C1*V2^E1+C2*V2+C2*(V-V2)^E2 /ez a keplet hibas a dokumentacioban/
		
		Fme(irodalmi)=2000+0.4*v(km/h)^2 [2/37,3/501]
	)
	Friction (
		1025N/m/s	-0.10		1.2mph		11.373N/m/s		1.907
		5.1N/rad/s		1		-1rad/s		0		1
	)
	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	
	MaxBrakeForce( 72kN ) comment ( V43 fektablazata alapjan: K: 10t, T: 42t, Sz: 72t, N: 107t )
	MaxHandbrakeForce( 10kN )

	EmergencyBrakeResMaxPressure( 55.1 ) comment ( Ilyen nincs valosagban a V43-ason, 3.8bar = 55.1psi )
	TripleValveRatio( 2.92 ) comment ( Dokumentacio szerint: 3.8bar[fekheng]/{5bar[fovez-toltott]-3.4[fovez-min]} [1/101],[4/284] )
	MaxReleaseRate( 11 ) comment  ( 5 s fekhenger uritesi ido 55psi/5s = 11psi/s csak mozdonyra /becsult/ )
	MaxApplicationRate( 18 ) comment ( 3 s fekhenger toltesi ido 55psi/3s = 18psi/s csak mozdonyra /becsult/ )
	MaxAuxilaryChargingRate( 40 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 40 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55.1 ) comment ( 3.8bar = 55.1psi )
	comment ( Irodalmi adat min. 4 bar [6/175] )

Lights ( 25
Comment ( 1 bal elso N+R )
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeF88017 )
     Position ( -0.83 1.52 7.24 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.6 )
     )
    )
   )
 Light (
  Comment ( 5 bal elso N+R REV )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeF88017 )
     Position ( -0.83 1.52 -7.24 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.6 )
     )
    )
   )
Comment ( 1 bal elso N+R1 )
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.83 1.52 7.242 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
 Light (
  Comment ( 5 bal elso N+R1 REV )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.83 1.52 -7.242 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )

Comment ( 1 bal elso T )
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 60ff7200 )
     Position ( -0.83 1.52 7.24 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.2 )
     )
    )
   )
Comment ( 1 bal elso T REV)
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 60ff7200 )
     Position ( -0.83 1.52 -7.24 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.2 )
     )
    )
   )
Comment ( 1 bal hatso T REV)
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 4 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 60ff7200 )
     Position ( -0.83 1.52 7.24 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.2 )
     )
    )
   )
Comment ( 1 bal hatso T )
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 1 )
    Unit ( 3 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 60ff7200 )
     Position ( -0.83 1.52 -7.24 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.2 )
     )
    )
   )
  Light (
  Comment ( 3 jobb elso N+R )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeF88017 )
     Position ( 0.83 1.52 7.24 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
  Light (
  Comment ( 5 jobb elso N+R REV )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeF88017 )
     Position ( 0.83 1.52 -7.24 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
  Light (
  Comment ( 3 jobb elso N+R1 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.83 1.52 7.242 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
  Comment ( 5 jobb elso N+R1 REV )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.83 1.52 -7.242 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
  Comment ( 11 fenycsova R )
   Type  ( 1 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.1 )
   FadeOut ( 0.3 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.0 0.5 7.3 )
     Transition ( 0 )
     Radius ( 80.0 )
     Angle ( 7.0 )
     )
    )
   )
  Light (
  Comment ( 12 fenycsova N )
   Type  ( 1 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.3 )
   FadeOut ( 0.1 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.0 1.0 7.5 )
     Transition ( 0 )
     Radius ( 150.0 )
     Angle ( 15.0 )
     )
    )
   )
  Light (
  Comment ( 13 tetofsz R )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0 3.61 7.07 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.7 )
     )
    )
   )
  Light (
  Comment ( 14 tetofsz R REV)
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0 3.61 -7.07 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.7 )
     )
    )
   )
  Light (
  Comment ( 15 bal hatso Z )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.63 1.51 -7.22 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
 Light (
  Comment ( 16 bal hatso Z REV)
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( -0.63 1.51 7.22 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
  Comment ( 17 jobb hatso Z )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( 0.63 1.51 -7.22 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
  Comment ( 18 jobb hatso Z REV)
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 4 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( 0.63 1.51 7.22 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
Comment ( AI fenyek 5 db )
Comment ( 1 bal elso N+R )
  Light (
   Type  ( 0 )
   Conditions (
				Control ( 1 )
        Unit ( 2 )
        Service ( 2 )
        TimeOfDay ( 0 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeF88017 )
     Position ( -0.83 1.52 7.25 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.6 )
     )
    )
   )
Comment ( 2 jobb elso N+R )
  Light (
   Type  ( 0 )
   Conditions (
				Control ( 1 )
        Unit ( 2 )
        Service ( 2 )
        TimeOfDay ( 0 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeF88017 )
     Position ( 0.83 1.52 7.25 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.6 )
     )
    )
   )
  Light (
  Comment ( 3 tetofsz R REV)
   Type  ( 0 )
   Conditions (
				Control ( 1 )
        Unit ( 2 )
        Service ( 2 )
        TimeOfDay ( 0 )    
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0 3.59 7.07 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.7 )
     )
    )
   )
  Light (
  Comment ( 4 jobb hatso Z )
   Type  ( 0 )
   Conditions (
				Control ( 1 )
        Unit ( 3 )
        Service ( 2 )
        TimeOfDay ( 0 )    
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( 0.63 1.51 -7.22 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
  Comment ( 5 bal hatso Z )
   Type  ( 0 )
   Conditions (
				Control ( 1 )
        Unit ( 3 )
        Service ( 2 )
        TimeOfDay ( 0 )    
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( -0.63 1.51 -7.22 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )

  )

 	Sound ( "H-MAVTR_V43c_eng.sms" )
)

Engine ( H-START_432-373
	Wagon ( H-START_432-373 )
	Type ( Electric )
	MaxPower ( 2200kW ) 
	MaxForce ( 350kN ) 
	MaxContinuousForce ( 310kN ) 
	MaxVelocity ( 120kmh ) comment ( [6/107], a vonatbefolyasolo berendezes miatt 120km/h )
	MaxCurrent ( 1500A ) comment ( Motoraramok 1700/1110/1070A indito/oras/allando [6/108] )
	WheelRadius ( 0.590m ) comment ( [6/107] )
	Sanding ( 1e2mph ) comment ( A homokolas nincs sebesseg alapjan korlatozva )
	NumWheels ( 2 ) comment ( Megfelelo tapadas elerese miatt fiktiv tengelyszam )

	CabView ( "v43_2xxx.cvf" )

	HeadOut ( 1.882 3.425 6.947 )

	AirBrakesAirCompressorPowerRating( 1.66 ) comment ( VV450/150 legsurito 2820l/min [6/110]= 1.66 ft3/s )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 145 ) comment ( 10bar = 145psi [6/110] )
	AirBrakesMainResVolume( 42.4 ) comment ( 2x600l = 42.4ft3 [6/189] )
	AirBrakesAirCompressorWattage( 19000 ) comment ( [6/109] )
	AirBrakesCompressorRestartPressure( 128 ) comment ( 8.8bar = 128 psi [6/158] )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.27 ) comment ( Levego igeny fontban. Jelentese nem teljesen vilagos. )
	AirBrakesIsCompressorElectricOrMechanical( 1 ) comment ( villamos legsurito )

	EngineBrakesControllerDirectControlExponent( 1 )
	EngineBrakesControllerMinPressureReduction( 4.35 ) comment( 5-4.7=0.3bar x 14.5=4.35psi )
	TrainBrakesControllerMinPressureReduction( 4.35 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 8 )
	TrainBrakesControllerMaxApplicationRate( 3.4 ) comment ( 23.2psi/6-8s[4/284]=3.87-2.9psi/s )
	EngineBrakesControllerMaxReleaseRate( 8 )
	TrainBrakesControllerMaxReleaseRate( 6.18 ) comment ( 23.2psi/3-5s[4/284]=7.73-4.64psi/s )
	EngineBrakesControllerEmergencyApplicationRate( 30 )
	TrainBrakesControllerEmergencyApplicationRate( 24 ) comment ( 58psi(5->1bar)/2-3s[4/285]=29-19.3psi/s )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72.5 ) comment ( fovezetek ny. 5bar=72.5 psi )
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 23.2 ) comment ( 5bar-3.4bar=1.6bar=23.2psi [4/284] )
	TrainBrakesControllerFullServicePressureDrop( 23.2 )
	comment ( VAGY: BrakeCylinderPressureForMaxBrakeBrakeForce[55.1]/TripleValveRatio[2.375]=23.2 ) 

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
  BrakesEngineControllers( "Independent, Train" )
	DoesBrakeCutPower( 0 )
	DoesHornTriggerBell( 0 )

    	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)
      VigilanceMonitor(
        MonitoringDeviceMonitorTimeLimit( 25 )
        MonitoringDeviceAlarmTimeLimit( 17 )
        MonitoringDevicePenaltyTimeLimit( 0 )
        MonitoringDeviceCriticalLevel( 0 )
        MonitoringDeviceResetLevel( 0 )
        MonitoringDeviceAppliesFullBrake( 1 )
        MonitoringDeviceAppliesEmergencyBrake( 0 )
        MonitoringDeviceAppliesCutsPower( 0 )
        MonitoringDeviceAppliesShutsDownEngine( 0 )
        )
      OverspeedMonitor(
        MonitoringDeviceMonitorTimeLimit( 0 )
        MonitoringDeviceAlarmTimeLimit( 5 )
        MonitoringDevicePenaltyTimeLimit( 0 )
        MonitoringDeviceCriticalLevel( 139 )
        MonitoringDeviceResetLevel( -1 )
        MonitoringDeviceAppliesFullBrake( 0 )
        MonitoringDeviceAppliesEmergencyBrake( 0 )
        MonitoringDeviceAppliesCutsPower( 0 )
        MonitoringDeviceAppliesShutsDownEngine( 0 )
        MonitoringDeviceTriggerOnTrackOverspeed( 0 )
        MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
        MonitoringDeviceResetOnZeroSpeed( 0 )
        MonitoringDeviceResetOnResetButton( 0 )
        )
  EngineControllers (
    Throttle ( 0 1 0.05 0 
      NumNotches ( 33
          Notch ( 0       0 Dummy )
          Notch ( 0.025   0 Dummy )
          Notch ( 0.050   0 Dummy )
          Notch ( 0.075   0 Dummy )
          Notch ( 0.100   0 Dummy )
          Notch ( 0.125   0 Dummy )
          Notch ( 0.150   0 Dummy )
          Notch ( 0.175   0 Dummy )
          Notch ( 0.200   0 Dummy )
          Notch ( 0.225   0 Dummy )
          Notch ( 0.250   0 Dummy )
          Notch ( 0.275   0 Dummy )
          Notch ( 0.300   0 Dummy )
          Notch ( 0.325   0 Dummy )
          Notch ( 0.350   0 Dummy )
          Notch ( 0.375   0 Dummy )
          Notch ( 0.400   0 Dummy )
          Notch ( 0.425   0 Dummy )
          Notch ( 0.450   0 Dummy )
          Notch ( 0.475   0 Dummy )
          Notch ( 0.500   0 Dummy )
          Notch ( 0.525   0 Dummy )
          Notch ( 0.550   0 Dummy )
          Notch ( 0.575   0 Dummy )
          Notch ( 0.600   0 Dummy )
          Notch ( 0.625   0 Dummy )
          Notch ( 0.650   0 Dummy )
          Notch ( 0.675   0 Dummy )
          Notch ( 0.700   0 Dummy )
          Notch ( 0.800   0 Dummy )
          Notch ( 0.900   0 Dummy )
          Notch ( 0.950   0 Dummy )
          Notch ( 1       0 Dummy )
          )
    )
  Brake_Train ( 0 1 0.1 0.4
    NumNotches ( 5
        Notch ( 0    0 TrainBrakesControllerReleaseStart )
        Notch ( 0.1  0 TrainBrakesControllerHoldStart )
        Notch ( 0.2  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
        Notch ( 0.9  0 TrainBrakesControllerContinuousServiceStart )
        Notch ( 1.0  0 TrainBrakesControllerEmergencyStart )
        )
    )
  Brake_Engine ( 0 1 0.03 0 
    NumNotches ( 1
        Notch ( 0    1 Dummy )
        )
    )
  DirControl ( -1 0 1 1 )
  EmergencyStopToggle( 0 1 0 )
  AWS ( 0 1 0 )
  Sanding ( 0 1 0 )
  Horn ( 0 1 0 )
  Vigilance ( 0 1 0 )
  PantographToggle1 ( 0 1 0 ) 
  PantographToggle2 ( 0 1 0 ) 
  Headlights ( 0 0.25 1 0 )
  Wipers ( 0 1 0 )
  BellToggle( 0 1 0 )
  BailOffButton( 0 1 0 )
  )
 Description (
	"The V43 series is an electric locomotive with Silicone Diode Rectifier (SDR). Built in 1963.\n\n"+
	"This electric engines are the most popular engines of the Hungarian State Railways (MÁV).\n\n"+
	"Power source: Overhead cable. (25 kV/50 Hz)\n\n"+
	"Power: 2,200 Kilowatts.\n\n"+
	"Max. speed: 130 km/h.\n\n"+
	"Height: 4.540 m\n\n"+
	"Width: 3.106 m\n\n"+
	"Length (Between bumpers): 15.700 m\n\n"+
	"Weight: 80.0 Metric Tons\n\n"+
	"Wheel configuration: Four wheels, in B'B' configuration."
 )
 EngineOperatingProcedures (
  "To move forward\n"+
  "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
	"2.	Press the W key to move the Reverser to Forward.\n"+
	"3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"4. 	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"5.	Press the D key to move increase the Throttle setting.\n\n"+  
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
	"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Press the ; (SEMICOLON) key and the [ (LEFT BRACKET) key to release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the 'permission to depart' signal.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
 ) 
 	Sound ( "H-MAVTR_V43c_cab.sms" )
)
