SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( V43-3216_2009
	

	Type ( Engine )
	WagonShape ( V43-3216_2009.s )
	FreightAnim ( V43-3216_2009_extra.s 1 1 )	
	Size ( 3.28m 4.5m 15.8m ) comment ( Szelesseg x Magassag x Hosszusag = 3106 x 4540 x 15700 mm [6/107] )
	CentreOfGravity ( 0m 0m 0m )
	Mass ( 80t ) comment ( [6/107] )
	WheelRadius ( 0.590m ) comment ( [6/107] )
	InertiaTensor ( Box ( 3.28m 4.5m 15.8m ) )
	comment( A megallaskor torteno visszarugas "szimulalasara" csokkentettem a rugoallandot )
	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
	CouplingHasRigidConnection ( 0 )
	Velocity ( 0.01m/s )
	)
	
comment ( Front Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
        CouplingHasRigidConnection ( 0 )
        Velocity ( 0.01m/s )
	)

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.1 0.36 1 0 ) comment ( MSTS default ertekek )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 400*2.5t )
	DerailBufferForce ( 2000kN )
	NumWheels ( 4 )	comment ( 4 tengelyes a mozdony B'B' tengelyelrendezessel [6/107] )
	comment ( MSTS menetellenallas parameterek jelentese a dokumentacio alapjan:
			C1		E1		V2		C2		E2
		C1,C2,E1,E2 konstansok, V2 sebesseghatar m/s (elso sor) vagy rad/s-ban (masodik sor)
		V aktualis sebesseg
		Ha V=<V2, akkor Fme(MSTS)=C1*V^E1
		Ha V>V2, akkor Fme(MSTS)=C1*V2^E1+C2*V2+C2*(V-V2)^E2 /ez a keplet hibas a dokumentacioban/
		
		Fme(irodalmi)=2000+0.4*v(km/h)^2 [2/37,3/501]
	)
	Friction (
		1025N/m/s	-0.10		1.2mph		11.373N/m/s		1.907
		5.1N/rad/s		1		-1rad/s		0		1

	)
#	AntiSlip ()

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	
	MaxBrakeForce( 72kN ) comment ( V43 fektablazata alapjan: K: 10t, T: 42t, Sz: 72t, N: 107t )
	MaxHandbrakeForce( 10kN )
#	NumberOfHandbrakeLeverSteps()

	EmergencyBrakeResMaxPressure( 55.1 ) comment ( Ilyen nincs valosagban a V43-ason, 3.8bar = 55.1psi )
#	TrainPipeLeakRate()
#	AuxilaryLeakRate()
	TripleValveRatio( 2.92 ) comment ( Dokumentacio szerint: 3.8bar[fekheng]/{5bar[fovez-toltott]-3.4[fovez-min]} [1/101],[4/284] )
	MaxReleaseRate( 11 ) comment  ( 5 s fekhenger uritesi ido 55psi/5s = 11psi/s csak mozdonyra /becsult/ )
	MaxApplicationRate( 18 ) comment ( 3 s fekhenger toltesi ido 55psi/3s = 18psi/s csak mozdonyra /becsult/ )
	MaxAuxilaryChargingRate( 40 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 40 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55.1 ) comment ( 3.8bar = 55.1psi )
		comment ( Irodalmi adat min. 4 bar [6/175] )

Lights ( 16
Comment ( 1bef )
  Light (
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.86 1.46 7.38 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 2bev )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 4 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( -0.64 1.46 7.36 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 3jef )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.86 1.46 7.38 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 4jev )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 4 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( 0.64 1.46 7.36 )
     Azimuth ( 0 0 0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 5bhf )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.86 1.46 -7.38 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 6bhv )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 3 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( -0.64 1.46 -7.36 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 7jhf )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.86 1.46 -7.38 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 8jhv )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 3 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( 0.64 1.46 -7.36 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 9nf )
   Type  ( 1 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.0 3.5 4 )
     Transition ( 0 )
     Radius ( 300.0 )
     Angle ( 15.0 )
     )
    )
   )


  Light (
  Comment ( 10tf )
   Type  ( 1 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -2.0 2.0 2 )
     Transition ( 0 )
     Radius ( 50.0 )
     Angle ( 7.0 )
     )
    )
   )


  Light (
  Comment ( 12jenr )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0 3.72 7.23 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 13betr )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.86 1.46 7.38 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 14jetr )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 5 )
    )
   FadeIn ( 0.8 )
   FadeOut ( 0.8 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( -0.86 1.46 7.38 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 16jhnr )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.8 )
   FadeOut ( 0.8 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0 3.72 -7.23 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 17bhtr )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   FadeIn ( 0.8 )
   FadeOut ( 0.8 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.86 1.46 -7.38 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )


  Light (
  Comment ( 18jhtr)
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 5 )
    )
   FadeIn ( 0.8 )
   FadeOut ( 0.8 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( eeffe095 )
     Position ( 0.86 1.46 -7.38 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
 )


    	Sound ( "H-MAVTR_V43-3x_eng.sms" )
)

Engine ( V43-3216_2009
	Wagon ( V43-3216_2009 )
	Type ( Electric )
	
	MaxPower ( 2200kW ) 
	MaxForce ( 310kN ) 
	MaxContinuousForce ( 310kN ) 
	MaxVelocity ( 130kmh ) comment ( [6/107], a vonatbefolyasolo berendezes miatt 120km/h )
	MaxCurrent ( 1400A ) comment ( Motoraramok 1700/1110/1070A indito/oras/allando [6/108] )
	WheelRadius ( 0.590m ) comment ( [6/107] )
	Sanding ( 1e2mph ) comment ( A homokolas nincs sebesseg alapjan korlatozva )
	NumWheels ( 2 ) comment ( Megfelelo tapadas elerese miatt fiktiv tengelyszam )

	CabView ( v43_3xxx.cvf )

	HeadOut ( 1.882 3.425 6.947 )

#	AirBrakeMaxMainResPipePressure( 145 )
	AirBrakesAirCompressorPowerRating( 1.66 ) comment ( VV450/150 legsurito 2820l/min [6/110]= 1.66 ft3/s )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 145 ) comment ( 10bar = 145psi [6/110] )
	AirBrakesMainResVolume( 42.4 ) comment ( 2x600l = 42.4ft3 [6/189] )
	AirBrakesAirCompressorWattage( 19000 ) comment ( [6/109] )
	AirBrakesCompressorRestartPressure( 128 ) comment ( 8.8bar = 128 psi [6/158] )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.27 ) comment ( Levego igeny fontban. Jelentese nem teljesen vilagos. )
#	AirBrakesHasLowPressureTest( 0 )
	AirBrakesIsCompressorElectricOrMechanical( 1 ) comment ( villamos legsurito )

	EngineBrakesControllerDirectControlExponent( 1 )

	EngineBrakesControllerMinPressureReduction( 4.35 ) comment( 5-4.7=0.3bar x 14.5=4.35psi )
	TrainBrakesControllerMinPressureReduction( 4.35 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 8 )
	TrainBrakesControllerMaxApplicationRate( 3.4 ) comment ( 23.2psi/6-8s[4/284]=3.87-2.9psi/s )
	EngineBrakesControllerMaxReleaseRate( 8 )
	TrainBrakesControllerMaxReleaseRate( 6.18 ) comment ( 23.2psi/3-5s[4/284]=7.73-4.64psi/s )
	EngineBrakesControllerEmergencyApplicationRate( 30 )
	TrainBrakesControllerEmergencyApplicationRate( 24 ) comment ( 58psi(5->1bar)/2-3s[4/285]=29-19.3psi/s )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72.5 ) comment ( fovezetek ny. 5bar=72.5 psi )
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 23.2 ) comment ( 5bar-3.4bar=1.6bar=23.2psi [4/284] )
	TrainBrakesControllerFullServicePressureDrop( 23.2 )
		comment ( VAGY: BrakeCylinderPressureForMaxBrakeBrakeForce[55.1]/TripleValveRatio[2.375]=23.2 ) 

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
         	
        BrakesEngineControllers( "Independent, Train" )
	DoesBrakeCutPower( 0 )
	DoesHornTriggerBell( 0 )
#	BrakeCutsPowerAtBrakeCylinderPressure( 15 )

    	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)
		
	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 25 )
		MonitoringDeviceAlarmTimeLimit( 17 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 139 )
		MonitoringDeviceResetLevel( -1 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 0 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 0 )
		MonitoringDeviceResetOnResetButton( 0 )
		)
	
        EngineControllers (
	   
            Throttle ( 0 1 0.05 0 
                NumNotches ( 33
                    Notch ( 0       0 Dummy )
                    Notch ( 0.025   0 Dummy )
                    Notch ( 0.050   0 Dummy )
                    Notch ( 0.075   0 Dummy )
			  Notch ( 0.100   0 Dummy )
                    Notch ( 0.125   0 Dummy )
                    Notch ( 0.150   0 Dummy )
			  Notch ( 0.175   0 Dummy )
                    Notch ( 0.200   0 Dummy )
                    Notch ( 0.225   0 Dummy )
			  Notch ( 0.250   0 Dummy )
                    Notch ( 0.275   0 Dummy )
                    Notch ( 0.300   0 Dummy )
                    Notch ( 0.325   0 Dummy )
                    Notch ( 0.350   0 Dummy )
                    Notch ( 0.375   0 Dummy )
                    Notch ( 0.400   0 Dummy )
                    Notch ( 0.425   0 Dummy )
                    Notch ( 0.450   0 Dummy )
                    Notch ( 0.475   0 Dummy )
                    Notch ( 0.500   0 Dummy )
                    Notch ( 0.525   0 Dummy )
                    Notch ( 0.550   0 Dummy )
   	 	        Notch ( 0.575   0 Dummy )
                    Notch ( 0.600   0 Dummy )
                    Notch ( 0.625   0 Dummy )
			  Notch ( 0.650   0 Dummy )
			  Notch ( 0.675   0 Dummy )
			  Notch ( 0.700   0 Dummy )
                    Notch ( 0.800   0 Dummy )
                    Notch ( 0.900   0 Dummy )
                    Notch ( 0.950   0 Dummy )
                    Notch ( 1       0 Dummy )
			)
            )
            Brake_Train ( 0 1 0.1 0.4
                  NumNotches ( 5
                    Notch ( 0    0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.1  0 TrainBrakesControllerHoldStart )
                    Notch ( 0.2  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 1.0  0 TrainBrakesControllerEmergencyStart )

                )
            )

            Brake_Engine ( 0 1 0.03 0 
                NumNotches ( 1
                    Notch ( 0    1 Dummy )
                )
            )
            
            DirControl ( -1 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 ) 
            PantographToggle2 ( 0 1 0 ) 
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
        )
        Name ( "H-MAV TR V43-3216_2009" )
        Description (
	"The V43 series is an electric locomotive with Silicone Diode Rectifier (SDR). Built in 1963.\n\n"+
	"This electric engines are the most popular engines of the Hungarian State Railways (MÁV).\n\n"+
	"Power source: Overhead cable. (25 kV/50 Hz)\n\n"+
	"Power: 2,200 Kilowatts.\n\n"+
	"Max. speed: 130 km/h.\n\n"+
	"Height: 4.540 m\n\n"+
	"Width: 3.106 m\n\n"+
	"Length (Between bumpers): 15.700 m\n\n"+
	"Weight: 80.0 Metric Tons\n\n"+
	"Wheel configuration: Four wheels, in B'B' configuration."
        )
        EngineOperatingProcedures (
        "To move forward\n"+
        "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
	"2.	Press the W key to move the Reverser to Forward.\n"+
	"3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"4. 	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"5.	Press the D key to move increase the Throttle setting.\n\n"+  
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
		"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Press the ; (SEMICOLON) key and the [ (LEFT BRACKET) key to release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the 'permission to depart' signal.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
        ) 
    	Sound ( "H-MAVTR_V43-3x_cab.sms" )
)

