SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( Vectron_170-044
 Type ( Carriage )
 WagonShape ( Vectron_170-044.s )
 FreightAnim ( Vectron_170-044_anim.s 1 1 )
 Size ( 3m 4m 19.42m )
 CentreOfGravity ( 0m 1.668m 0m )
 Mass ( 87t )
 WheelRadius ( 0.625m )
 InertiaTensor ( Box ( 3m 4m 19m ) )
 Coupling (
 Type ( Chain )
 Spring (
  Stiffness ( 1.1e6N/m 4.8e6N/m )
  Damping ( 1.2e6N/m/s 3.4e6N/m/s )
  Break ( 3.4e7N 3.4e7N )
  r0 ( 20cm 30cm )
  )
 CouplingHasRigidConnection ( )
 Velocity ( 0.15m/s )
 )
 Coupling (
 Type ( Chain )
 Spring (
  Stiffness ( 4.8e6N/m 1.1e6N/m )
  Damping ( 3.4e6N/m/s 1.2e6N/m/s )
  Break ( 3.4e7N 3.4e7N )
  r0 ( 30cm 20cm )
  )
 CouplingHasRigidConnection ( )
 Velocity ( -0.15m/s )
 )
 Buffers (
 Spring (
  Stiffness ( 1e7N/m 0 )
  Damping ( 1e6N/m/s 0 )
  r0 ( 0m 1e9 )
  )
 Centre ( 0.5m )
 Radius ( 1m )
 Angle ( 0.5deg )
 )
 Adheasion ( 0.25 0.44 2 0 )
 DerailRailHeight ( 5cm )
 DerailRailForce ( 435kN )
 DerailBufferForce ( 250kN )
 NumWheels ( 1 )
 Friction (
 comment( values by Joseph Realmuto FCalc 2.0 )
 comment( entered values are: L,F,R,4,87,11,0.6;Y,87 )
 1070.5N/m/s -0.10 1.2mph 8.893N/m/s 1.822
 5.1N/rad/s 1 -1rad/s 0 1
 )
 AntiSlip ( )
 BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Emergency_reservoir" )
 BrakeSystemType ( "Air_single_pipe" )
 MaxBrakeForce( 180kN )

 EmergencyBrakeResMaxPressure( 72 )
 TripleValveRatio( 3 )
 MaxReleaseRate( 4 )
 MaxApplicationRate( 5 )
 MaxAuxilaryChargingRate( 5 )
 EmergencyResCapacity( 4 )
 EmergencyResChargingRate( 5 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 54 )
 BrakeAirPressureGainInResForOnePoundFromPipe( 0.5 )

   Sound ( "GenFreightWag1.sms" )
)
