SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 
 193-872
 Type ( Engine )
 WagonShape ( 193-872.s )
 FreightAnim ( 193-872_anim.s 1 1 )
 Size ( 3m 4m 19.42m )
 CentreOfGravity ( 0m 1.668m 0m )
 Mass ( 87t )
 WheelRadius ( 0.625m )
 InertiaTensor (
  Box ( 3m 4m 19m )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 1.1e6N/m 4.8e6N/m )
   Damping ( 1.2e6N/m/s 3.4e6N/m/s )
   Break ( 3.4e7N 3.4e7N )
   r0 ( 20cm 30cm )
  )
  CouplingHasRigidConnection ()
  Velocity ( 0.15m/s )
 )
 Coupling (
  Type ( Chain )
  Spring (
   Stiffness ( 4.8e6N/m 1.1e6N/m )
   Damping ( 3.4e6N/m/s 1.2e6N/m/s )
   Break ( 3.4e7N 3.4e7N )
   r0 ( 30cm 20cm )
  )
  CouplingHasRigidConnection ()
  Velocity ( -0.15m/s )
 )
 Buffers (
  Spring (
   Stiffness ( 1e7N/m 0 )
   Damping ( 1e6N/m/s 0 )
   r0 ( 0m 1e9 )
  )
  Centre ( 0.5m )
  Radius ( 1m )
  Angle ( 0.5deg )
 )
 Adheasion ( 0.25 0.44 2 0 )
 DerailRailHeight ( 5cm )
 DerailRailForce ( 435kN )
 DerailBufferForce ( 250kN )
 NumWheels ( 1 )
 Friction (
  comment ( values by Joseph Realmuto FCalc 2.0 )
  comment ( entered values are: L,F,R,4,87,11,0.6;Y,87 )
  1070.5N/m/s -0.10 1.2mph 8.893N/m/s 1.822 5.1N/rad/s 1 -1rad/s 0 1 
 )
 AntiSlip ()
 BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Emergency_reservoir" )
 BrakeSystemType ( "Air_single_pipe" )
 MaxBrakeForce ( 180kN )
 EmergencyBrakeResMaxPressure ( 72 )
 TripleValveRatio ( 3 )
 MaxReleaseRate ( 4 )
 MaxApplicationRate ( 5 )
 MaxAuxilaryChargingRate ( 5 )
 EmergencyResCapacity ( 4 )
 EmergencyResChargingRate ( 5 )
 BrakeCylinderPressureForMaxBrakeBrakeForce ( 54 )
 BrakeAirPressureGainInResForOnePoundFromPipe ( 0.5 )
 Lights (
  14 
  Light (
   comment ( TOP Sphere of light )
   Type ( 1 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
   )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( ffffffff )
     Position ( 0.0 3.602 9.015 )
     Transition ( 0 )
     Radius ( 400.0 )
     Angle ( 15.0 )
    )
   )
  )
  Light (
   comment ( FRONT Head top light )
   Type ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( ffffffff )
     Position ( 0.15 3.671 8.9 )
     Azimuth ( 0 -15 0 )
     Elevation ( -50 -50 -50 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
  Light (
   comment ( FRONT Head top light )
   Type ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( ffffffff )
     Position ( -0.15 3.67 8.9 )
     Azimuth ( 0 0 15 )
     Elevation ( -50 -50 -50 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
  Light (
   comment ( FRONT left light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
   )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( aaffffff )
     Position ( -1.2 1.65 9.35 )
     Transition ( 0 )
     Radius ( 0.8 )
     Azimuth ( 0 -40 10 )
     Elevation ( 0 -25 25 )
    )
   )
  )
  Light (
   comment ( FRONT right light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
   )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( aaffffff )
     Position ( 1.2 1.65 9.35 )
     Transition ( 0 )
     Radius ( 0.8 )
     Azimuth ( 0 -10 40 )
     Elevation ( 0 -25 25 )
    )
   )
  )
  Light (
   comment ( FRONT left red light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 4 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( -1.2 1.9 9.39 )
     Azimuth ( 0 -40 10 )
     Elevation ( 0 -25 25 )
     Transition ( 0 )
     Radius ( 0.4 )
    )
   )
  )
  Light (
   comment ( FRONT right red light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 4 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( ffff0000 )
     Position ( 1.2 1.9 9.39 )
     Azimuth ( 0 -10 40 )
     Elevation ( 0 -25 25 )
     Transition ( 0 )
     Radius ( 0.4 )
    )
   )
  )
  Light (
   comment ( REAR Head top light )
   Type ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( ffffffff )
     Position ( 0.15 3.671 -8.9 )
     Azimuth ( -180 -170 -180 )
     Elevation ( -50 -50 -50 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
  Light (
   comment ( REAR Head top light )
   Type ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( ffffffff )
     Position ( -0.15 3.67 -8.9 )
     Azimuth ( -180 170 180 )
     Elevation ( -50 -50 -50 )
     Transition ( 0 )
     Radius ( 1.0 )
    )
   )
  )
  Light (
   comment ( REAR left light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
   )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( aaffffff )
     Position ( -1.2 1.65 -9.35 )
     Azimuth ( -180 -150 -180 )
     Elevation ( 0 -25 25 )
     Transition ( 0 )
     Radius ( 0.8 )
    )
   )
  )
  Light (
   comment ( REAR right light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
   )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States (
    1 
    State (
     Duration ( 0.0 )
     LightColour ( aaffffff )
     Position ( 1.2 1.65 -9.35 )
     Azimuth ( -180 150 180 )
     Elevation ( 0 -25 25 )
     Transition ( 0 )
     Radius ( 0.8 )
    )
   )
  )
  Light (
   comment ( REAR left red light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0 )
     LightColour ( FFFF0000 )
     Position ( -1.2 1.9 -9.39 )
     Azimuth ( -180 -180 -140 )
     Elevation ( 0 -25 25 )
     Transition ( 0 )
     Radius ( 0.4 )
    )
   )
  )
  Light (
   comment ( REAR right red light )
   Type ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States (
    1 
    State (
     Duration ( 0 )
     LightColour ( FFFF0000 )
     Position ( 1.2 1.9 -9.39 )
     Azimuth ( -180 140 180 )
     Elevation ( 0 -25 25 )
     Transition ( 0 )
     Radius ( 0.4 )
    )
   )
  )
  Light (
   comment ( Pantograph flash )
   Type ( 0 )
   Conditions (
    Headlight ( 0 )
    Unit ( 3 )
   )
   FadeIn ( 0 )
   FadeOut ( 0 )
   Cycle ( 0 )
   States (
    8 
    State (
     Duration ( 4.0 )
     LightColour ( 11000000 )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.90 )
     Elevation ( 0 -90 90 )
    )
    State (
     Duration ( 0.05 )
     LightColour ( ffaaaaff )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 1.30 )
     Elevation ( 0 -90 90 )
    )
    State (
     Duration ( 15.0 )
     LightColour ( 11000000 )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.90 )
     Elevation ( 0 -90 90 )
    )
    State (
     Duration ( 0.05 )
     LightColour ( ffaaaaff )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.90 )
     Elevation ( 0 -90 90 )
    )
    State (
     Duration ( 7.0 )
     LightColour ( 11000000 )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.90 )
     Elevation ( 0 -90 90 )
    )
    State (
     Duration ( 0.05 )
     LightColour ( ffaaaaff )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 1.1 )
     Elevation ( 0 -90 90 )
    )
    State (
     Duration ( 0.05 )
     LightColour ( 11000000 )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.90 )
     Elevation ( 0 -90 90 )
    )
    State (
     Duration ( 0.05 )
     LightColour ( ffaaaaff )
     Position ( 0.0 5.5 -5.3 )
     Azimuth ( 0.0 -180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.90 )
     Elevation ( 0 -90 90 )
    )
   )
  )
 )
 Sound ( "4700eng.sms" )
)
Engine (
 193-872 
 Wagon ( 193-872 )
 Type ( Electric )
 MaxPower ( 4684kW )
 MaxForce ( 300kN )
 MaxContinuousForce ( 250kN )
 MaxVelocity ( 87mph )
 MaxCurrent ( 300A )
 WheelRadius ( 0.625m )
 Sanding ( 6mph )
 NumWheels ( 1 )
 CabView ( "vectron.cvf" )
 HeadOut ( -1.7 3.0 7.75 )
 MaxTemperature ( 120 )
 MaxOilPressure ( 90 )
 AirBrakesAirCompressorPowerRating ( 3.5 )
 AirBrakesMainMinResAirPressure ( 0 )
 AirBrakesMainMaxAirPressure ( 72 )
 AirBrakesMainResVolume ( 28 )
 AirBrakesAirCompressorWattage ( 10000 )
 AirBrakesCompressorRestartPressure ( 67 )
 AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 1.5 )
 AirBrakesHasLowPressureTest ( 1 )
 AirBrakesIsCompressorElectricOrMechanical ( 0 )
 EngineBrakesControllerHasProportionalBrake ( 1 )
 EngineBrakesProportionalBrakeLag ( 1 )
 EngineBrakesControllerMaxApplicationRate ( 7 )
 EngineBrakesControllerMinSystemPressure ( 0 )
 EngineBrakesControllerMaxSystemPressure ( 72 )
 EngineBrakesControllerEmergencyBrakeTimePenalty ( 5 )
 EngineBrakesControllerFullServicePressureDrop ( 26 )
 EngineBrakesControllerMinPressureReduction ( 1 )
 EngineBrakesControllerMaxReleaseRate ( 7 )
 EngineBrakesControllerEmergencyApplicationRate ( 40 )
 EngineBrakesControllerDirectControlExponent ( 1 )
 TrainBrakesControllerMinPressureReduction ( 1 )
 TrainBrakesControllerMaxApplicationRate ( 10 )
 TrainBrakesControllerMaxReleaseRate ( 10 )
 TrainBrakesControllerEmergencyApplicationRate ( 40 )
 TrainBrakesControllerMinSystemPressure ( 0 )
 TrainBrakesControllerMaxSystemPressure ( 72 )
 TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
 TrainBrakesControllerFullServicePressureDrop ( 26 )
 DynamicBrakesMinUsableSpeed ( 5 )
 DynamicBrakesMaximumEffectiveSpeed ( 25 )
 DynamicBrakesMaximumForce ( 850kN )
 DynamicBrakesResistorCurrentLimit ( 326A )
 DynamicBrakesCutInSpeed ( 1 )
 DynamicBrakesMaxAirBrakePressure ( 55 )
 DynamicBrakesFadingSpeed ( 45 )
 DynamicBrakesDelayTimeBeforeEngaging ( 0 )
 DynamicBrakesMaximumSpeedForFadeOut ( 95 )
 DynamicBrakesEffectAtMaximumFadeOut ( 1 )
 DynamicBrakesHigherSpeedCurveExponent ( 1 )
 DynamicBrakesLowerSpeedCurveExponent ( 1 )
 DynamicBrakesNumberOfControllerNotches ( 11 )
 BrakesEngineBrakeType ( "Air_single_pipe" )
 BrakesTrainBrakeType ( "Air_single_pipe" )
 BrakesEngineControllers ( "Independent, Train, Dynamic" )
 DoesBrakeCutPower ( 1 )
 DoesHornTriggerBell ( 0 )
 DieselEngineSpeedOfMaxTractiveEffort ( 13mph )
 BrakeCutsPowerAtBrakeCylinderPressure ( 14 )
 EmergencyStopMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 0 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  MonitoringDeviceAppliesFullBrake ( 0 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 1 )
 )
 VigilanceMonitor (
  MonitoringDeviceMonitorTimeLimit ( 45 )
  MonitoringDeviceAlarmTimeLimit ( 37 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 0 )
  MonitoringDeviceResetLevel ( 0 )
  MonitoringDeviceAppliesFullBrake ( 1 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
 )
 OverspeedMonitor (
  MonitoringDeviceMonitorTimeLimit ( 0 )
  MonitoringDeviceAlarmTimeLimit ( 5 )
  MonitoringDevicePenaltyTimeLimit ( 0 )
  MonitoringDeviceCriticalLevel ( 97 )
  MonitoringDeviceResetLevel ( 0 )
  MonitoringDeviceAppliesFullBrake ( 1 )
  MonitoringDeviceAppliesEmergencyBrake ( 1 )
  MonitoringDeviceAppliesCutsPower ( 1 )
  MonitoringDeviceAppliesShutsDownEngine ( 0 )
  MonitoringDeviceTriggerOnTrackOverspeed ( 0 )
  MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
  MonitoringDeviceResetOnZeroSpeed ( 1 )
  MonitoringDeviceResetOnResetButton ( 1 )
 )
 EngineControllers (
  Throttle (
   0 1 0.034 0 
   NumNotches ( 0 )
  )
  Brake_Engine (
   0 1 0.125 0 
   NumNotches (
    3 
    Notch ( 0 0 EngineBrakesControllerReleaseStart )
    Notch ( 0.1 1 EngineBrakesControllerGraduatedSelfLapLimitedHoldingStart )
    Notch ( 0.95 0 EngineBrakesControllerFullServiceStart )
   )
  )
  Brake_Train (
   0 1 0.05 0.2 
   NumNotches (
    6 
    Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
    Notch ( 0.1 0 TrainBrakesControllerReleaseStart )
    Notch ( 0.2 0 TrainBrakesControllerHoldLappedStart )
    Notch ( 0.3 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
    Notch ( 0.9 0 TrainBrakesControllerContinuousServiceStart )
    Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
   )
  )
  Brake_Dynamic (
   0 1 0.01 0 
   NumNotches (
    11 
    Notch ( 0 0 Dummy )
    Notch ( 0.1 0 Dummy )
    Notch ( 0.2 0 Dummy )
    Notch ( 0.3 0 Dummy )
    Notch ( 0.4 0 Dummy )
    Notch ( 0.5 0 Dummy )
    Notch ( 0.6 0 Dummy )
    Notch ( 0.7 0 Dummy )
    Notch ( 0.8 0 Dummy )
    Notch ( 0.9 0 Dummy )
    Notch ( 1.0 0 Dummy )
   )
  )
  DirControl ( -1 0 1 1 )
  EmergencyStopResetToggle ( 0 1 0 )
  EmergencyStopToggle ( 0 1 0 )
  AWS ( 0 1 0 )
  Sanding ( 0 1 0 )
  Horn ( 0 1 0 )
  Vigilance ( 0 1 0 )
  PantographToggle1 ( 0 1 1 )
  PantographToggle2 ( 0 1 0 )
  PantographToggle_4 ( 0 1 1 )
  Headlights ( 0 0.25 1 2 )
  Wipers ( 0 1 0 )
  BellToggle ( 0 1 0 )
  BailOffButton ( 0 1 0 )
 )
 Sound ( "4700cab.sms" )
 Name ( "Vectron 193-872" )
 Description ( "Locomotiva Eléctrica de Via Larga\n"+
  "CP serie 4700\n"+
  "Locomotiva de Carga.\n\n"+
  "Potecia: 4600 kW\n\n"+
  "V. Max: 140 Km/h (87 mph)\n\n"+
  "Ano de Construcao 2007-2009\n\n"+
  "Entrada ao Servico: 2008" )
 EngineOperatingProcedures ( "To move forward\n"+
  "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
  "2. Press the W key to move the Reverser to Forward.\n"+
  "3. Press the ; (SEMICOLON) key to release the train brakes.\n"+
  "4. Press the D key to move increase the throttle setting.\n\n"+
  "To slow the train\n"+
  "1. Press the A key to move the throttle to a lower setting.\n"+
  "2. Use the brakes to further reduce speed if desired.\n\n"+
  "To apply the train brakes\n"+
  "1. Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
  "To release the train brakes\n"+
  "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
  "To activate emergency braking\n"+
  "1. Press the A key to reduce the throttle to Idle.\n"+
  "2. Press the BACKSPACE key to activate emergency braking.\n\n"+
  "To back up\n"+
  "1. Bring your train to a full stop.\n"+
  "2. Press the S key to move the Reverser to the Reverse position.\n"+
  "3. Press the ; (SEMICOLON)  to release the brakes.\n"+
  "4. Slowly advance the throttle lever (D key).\n\n"+
  "To load and unload passengers\n"+
  "1. Stop at a station.\n"+
  "2. Press the ENTER key.\n"+
  "3. Wait for the 'permission to depart' signal.\n"+
  "TIP: Use the Next Station driving aid (F10) to monitor loading and unloading." )
)
