SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-Start_2415-067_D
	Type ( Carriage )
	WagonShape ( H-Start_2415-067_D.s )
	comment ( Fiktív hossz használata a tökéletes kapcsolódás miatt )
	Name ( "H-Start_2415-067_D" )
        Size ( 2.914m 3.809m 6.1m )
	CentreOfGravity ( 0m 0m 0m )
	Mass ( 31.1t )
	WheelRadius ( 0.750m )
	InertiaTensor ( Box (2.914m 3.809m 6.1m) )
	comment ( Rear Coupler )
	Coupling (
		Type ( Bar )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
	CouplingHasRigidConnection ( 1 )
	Velocity ( 0.01m/s )
	)
	
comment ( Front Coupler )

	Coupling (
		Type ( Bar )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
        CouplingHasRigidConnection ( 1 )
        Velocity ( 0.01m/s )
	)

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.1 0.3 1.3 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 100kN )
	DerailBufferForce ( 100kN )
	NumWheels (	4 ) 
	Friction (
		721N/m/s	0	0mph	           0.1N/m/s     	1.8
		5.1N/rad/s	1          -1rad/s		0		1
    	)

	AntiSlip ( )
	
	BrakeEquipmentType ( "ep_brake" )
	BrakeSystemType ( EP )
	MaxBrakeForce ( 60kN )
	EmergencyBrakeResMaxPressure ( 60 )
	TripleValveRatio ( 2.5 )
	MaxReleaseRate ( 7 )
	MaxApplicationRate ( 5 )
	MaxAuxilaryChargingRate ( 5 )
	EmergencyResCapacity ( 7 )
	EmergencyResChargingRate ( 5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 60 )


	PassengerCapacity ( 53 )

        PantographToggle1 ( 0 1 0 ) 
        PantographToggle2 ( 0 1 0 ) 
        PantographsToggle_6 ( 0 1 3 )

Sound  ( Flirt_eng00.sms )


)
