SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-Start_2415-069_C_AI
	

	Type ( Engine )
	WagonShape ( H-Start_2415-069_C.s )	
	Size ( 2.914m 3.809m 6.5m )
	comment( Fiktív méretmeghatározás csatlás helyessége miatt )
	CentreOfGravity ( 0m 0m 0.0m )
	Mass ( 31.7t ) 
	WheelRadius ( 0.850m ) 
	InertiaTensor ( Box ( 2.914m 3.809m 6.5m ) )

  comment ( Rear Coupler )
	Coupling (
		Type ( Bar )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
	CouplingHasRigidConnection ( 1 )
	Velocity ( 0.01m/s )
	)
	
comment ( Front Coupler )

	Coupling (
		Type ( Bar )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
        CouplingHasRigidConnection ( 1 )
        Velocity ( 0.01m/s )
	)

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.1 0.36 2 0 ) comment ( MSTS default ertekek )
	DerailRailHeight ( 4cm )
 	DerailRailForce ( 310kN )
	DerailBufferForce ( 310kN )
	NumWheels ( 4 )	
	Friction (
		721N/m/s	0	1mph	           2.51N/m/s     	1.8
		5.1N/rad/s	1          -1rad/s		0		1
    	)
	AntiSlip ()

	BrakeEquipmentType( "EP_brake" )
	BrakeSystemType( "EP" )
	
	MaxBrakeForce( 140kN )
	MaxHandbrakeForce( 20kN )

	EmergencyBrakeResMaxPressure( 55.1 )
	TripleValveRatio( 2.92 )
	MaxReleaseRate( 7 )
	MaxApplicationRate( 11 )
	MaxAuxilaryChargingRate( 40 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 40 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55.1 )
	PassengerCapacity ( 80 )	
	    	Sound ( "Flirt_eng00.sms" )
)

Engine ( H-Start_2415-069_C_AI
	Wagon ( H-Start_2415-069_C_AI )
	Type ( Electric )
	
	MaxPower ( 10kW ) 
	MaxForce ( 1kN ) 
	MaxContinuousForce ( 1kN ) 
	MaxVelocity ( 160kmh )
	MaxCurrent ( 1A ) 
	WheelRadius ( 0.850m ) 
	Sanding ( 1kmph )
	NumWheels ( 1 )

	

          EngineControllers (
            Throttle ( 0 1 0.05 0 
                NumNotches ( 0 )
            )
            )
            Combined_Control( 0 1 0.125 0 throttle dynamic )
            DirControl ( -1 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Horn ( 0 1 0 )
            PantographToggle1 ( 0 1 0 ) 
            PantographToggle2 ( 0 1 0 ) 
            PantographsToggle_6 ( 0 1 3 ) 
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
        )
        Name ( "H-Start_2415-069_C_AI" )
        Description ( H-Start FLIRT )
        EngineOperatingProcedures (
        "To move forward\n"+
        "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
	"2.	Press the W key to move the Reverser to Forward.\n"+
	"3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"4. 	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"5.	Press the D key to move increase the Throttle setting.\n\n"+  
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
		"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Press the ; (SEMICOLON) key and the [ (LEFT BRACKET) key to release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the 'permission to depart' signal.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
        ) 
            	Sound ( "Flirt_cab.sms" )
)
