SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-Start_5342_002-2_B
	Type ( Engine )
	WagonShape ( H-Start_5342_002-2_B.s )
	Size  ( 2.925m 3.360m 18.65m )
	CentreOfGravity ( 0m 1.7m 0m )
	MaxTilt ( 6.5deg )
	Mass ( 30t )
	WheelRadius ( 0.475m )
	InertiaTensor ( Box (2.9m 3.3m 18.65m) )
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 2e5N/m 0 )
			Damping ( 2e5N/m/s 0 )
			Break ( 3e7N 0 )
			r0 ( 15cm 15cm )
		)
		CouplingHasRigidConnection ( 1 )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 2e5N/m 0  )
			Damping ( 2e5N/m/s 0 )
			Break ( 3e7N 0 )
			r0 ( 0.1 1e9 )
		)
		CouplingHasRigidConnection ( 1 )
	)
	Buffers (
		Spring (
			Stiffness ( 1e8N/m 0N/m )
			Damping ( 1e8N/m/s 0N/m/s)
			r0 ( 0m 1e9 )
		)
		Centre ( 1 )
		Radius ( 2 )
		Angle ( 1deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 7cm )
	DerailRailForce ( 77.1kN )
	DerailBufferForce ( 294kN )
	NumWheels ( 3 )					comment ( Räder )
	Friction (
		491.5N/m/s		-0.05		1mph		7.163N/m/s		1.95
		5.1N/rad/s		1		-1rad/s		0		1
	)
	AntiSlip ()


	BrakeEquipmentType( "EP_brake" )
	BrakeSystemType( "EP" )
	
	MaxBrakeForce( 180kN )
	MaxHandbrakeForce( 10kN )

	EmergencyBrakeResMaxPressure( 55.1 )
	TripleValveRatio( 2.92 )
	MaxReleaseRate( 7 )
	MaxApplicationRate( 7 )
	MaxAuxilaryChargingRate( 40 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 40 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55.1 )

	PassengerCapacity ( 73 )
	

Sound ( "talent_eng.sms" )

	Lights	( 14
		
Light (
comment( Sphere of light Mid )
Type ( 1 )
Conditions (
Headlight ( 2 )
Unit ( 2 )
)
Cycle ( 0 )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State (
Duration ( 0.0 )
LightColour ( eeffe095 )
Position ( 0.0 1 6.4 )
Transition ( 0 )
Radius ( 80.0 )
Angle ( 16.0 )
)
)
)
Light (
comment( Sphere of light Full )
Type ( 1 )
Conditions (
Headlight ( 3 )
Unit ( 2 )
)
Cycle ( 0 )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State (
Duration ( 0.0 )
LightColour ( eeffe095 )
Position ( 0.0 1.4 18 )
Transition ( 0 )
Radius ( 160.0 )
Angle ( 12.0 )
)
)
)


				Light	(
			comment( bal elso feher DIM+FULL1 )
			Type			( 0 )
			Conditions (
				Headlight 	( 4 )
				Unit 		( 2 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( -0.44 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)

		Light	(
			comment( bal elso feher FULL2 )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( -0.66 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb elso feher DIM+FULL )
			Type			( 0 )
			Conditions (
				Headlight 	( 4 )
				Unit 		( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( 0.44 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb elso feher FULL2 )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( 0.66 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( REFI )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( 0.0 3.67 7.2 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal hatso voros FULL REV )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( ffff0000 )
					Position 	( -0.66 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb hatso voros FULL REV)
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( ffff0000 )
					Position 	( 0.66 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)

		Light	(
			comment( bal elso feher FULL1 AI )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( -0.44 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( REFI FULL1 AI )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( -0.0 3.68 7.2 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal elso feher FULL2 AI)
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( -0.66 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb elso feher FULL1 AI )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( 0.44 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal elso feher FULL2 AI)
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFAFDB8 )
					Position 	( 0.66 2.18 8.725 )
					Azimuth 	( 0.0 0.0 0.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
)
)


    Engine ( H-Start_5342_002-2_B
    Wagon ( H-Start_5342_002-2_B )
    Type ( Electric )
    MaxPower ( 860kW )
    MaxForce ( 70kN )
    MaxContinuousForce ( 180kN )
    MaxVelocity ( 140km/h )
    MaxCurrent ( 800A )
    WheelRadius ( 0.475m )
    Sanding ( 1e9mph )
    NumWheels ( 3 )

    CabView ( 4023_a.cvf )

	AirBrakeMaxMainResPipePressure( 145 )
	AirBrakesAirCompressorPowerRating( 3.45 ) 
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 145 ) 
	AirBrakesMainResVolume( 42.4 )
	AirBrakesAirCompressorWattage( 19000 )
	AirBrakesCompressorRestartPressure( 128 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.27 )
#	AirBrakesHasLowPressureTest( 0 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerDirectControlExponent( 1 )

	EngineBrakesControllerMinPressureReduction( 4.35 )
	TrainBrakesControllerMinPressureReduction( 4.35 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 8 )
	TrainBrakesControllerMaxApplicationRate( 5.2 ) 
	EngineBrakesControllerMaxReleaseRate( 8 )
	TrainBrakesControllerMaxReleaseRate( 2.5 )
	EngineBrakesControllerEmergencyApplicationRate( 30 )
	TrainBrakesControllerEmergencyApplicationRate( 24 )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72.5 )
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 23.2 )
	TrainBrakesControllerFullServicePressureDrop( 23.2 )

	DynamicBrakesMinUsableSpeed ( 5kph )
	DynamicBrakesMaximumEffectiveSpeed ( 999 )
	DynamicBrakesMaximumForce ( 70kN )
	DynamicBrakesResistorCurrentLimit ( 5000 )
	DynamicBrakesCutInSpeed ( 0mph )
	DynamicBrakesMaxAirBrakePressure ( 70 )
	DynamicBrakesFadingSpeed ( 10kph )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
	DynamicBrakesMaximumSpeedForFadeOut ( 999 )
	DynamicBrakesEffectAtMaximumFadeOut ( 110 )
	DynamicBrakesHigherSpeedCurveExponent ( 1 )
	DynamicBrakesLowerSpeedCurveExponent ( 1 )
	DynamicBrakesNumberOfControllerNotches ( 0 )


	DoesHornTriggerBell( 0 )

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 38 )
		MonitoringDeviceAlarmTimeLimit ( 30 )
		MonitoringDevicePenaltyTimeLimit ( 5 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 0 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		)

          EngineControllers (
            Throttle ( 0 1 0.05 0 
                NumNotches ( 0 )
            )
            Brake_Dynamic ( 0 1 0.15 0 
                NumNotches ( 0 ) 
	    )
            Brake_Train ( 0 1 0.1 0
                NumNotches ( 4
                    Notch ( 0    0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.1  0 TrainBrakesControllerEPApplyStart )
                    Notch ( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 1.0  0 TrainBrakesControllerEmergencyStart )
                )
            )
            Combined_Control( 0 1 0.125 0 throttle dynamic )
            EmergencyStopToggle( 0 1 0 )
            EmergencyStopResetToggle( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
        )

        Name ( "H-Start_5342_002-2_B" )
        Description ( H-Start_5342_002-2_B  )
	EngineOperatingProcedures (
	"So setzen Sie den Zug in Bewegung\n"+
	"1. Drücken Sie die P-TASTE, um den Stromabnehmer auszufahren.\n"+	
	"2.	Drücken Sie die D-TASTE, um den Hauptsteuerhebel in die Position Leerlauf zu stellen.\n"+
	"	Hinweis: Wenn sich der Hauptsteuerhebel in der Stellung Leerlauf befindet, leuchtet eine grünes Licht auf.\n"+
	"3.	Drücken Sie die W-TASTE, um den Richtungshebel auf  Vorwärts zu stellen.\n"+
	"	Hinweis: Der Richtungshebel kann nur bedient werden, wenn sich der Regler in der Stellung Leerlauf befindet.\n"+
	"4.	Drücken Sie die D-TASTE, um den Hauptsteuerhebel in die Reglerkerbe 1 zu stellen.\n"+
	"5.	Wenn Sie schneller fahren möchten, drücken Sie die D-TASTE, um den Hauptsteuerhebel in eine höhere Reglerkerbe zu bewegen.\n"+
	"So bremsen Sie den Zug ab\n"+
	"1.	Drücken Sie die A-TASTE, um den Regler nach unten zu bewegen.\n"+
	"2.	Setzen Sie die Bremsen ein, wenn Sie noch weiter abbremsen möchten.\n\n"+   
	"So bedienen Sie die Zugbremsen\n"+
	"1.	Drücken Sie die A-TASTE, um die Zugbremsen anzulegen.\n\n"+
	"So lösen Sie die Zugbremsen\n"+
	"1. Drücken Sie die D-TASTE, um die Zugbremsen zu lösen.\n\n"+
	"So lösen Sie die Notbremse aus\n"+
	"1.	Drücken Sie die A-TASTE, um den Hauptsteuerhebel zur höchsten Bremseinstellung zu bewegen.\n"+
	"	- oder -\n"+
	"2.	Drücken Sie die RÜCKTASTE.\n\n"+
	"So fahren Sie rückwärts\n"+
	"1.	Halten Sie den Zug vollständig an.\n"+ 
	"2.	Drücken Sie die S-TASTE, um den Richtungshebel in die Position Rückwärts zu stellen.\n"+
	"	Hinweis: Der Richtungshebel kann nur bedient werden, wenn sich der Regler in der Stellung Leerlauf befindet.\n"+
	"4.	Drücken Sie die Ö-TASTE, um die Bremsen zu lösen.\n"+
	"5.	Schieben Sie den Regler langsam nach vorne (D-TASTE).\n\n"+
	"So lassen Sie Fahrgäste ein- und aussteigen\n"+
	"1. Halten Sie an einem Bahnhof an.\n"+
	"2. Drücken Sie die EINGABETASTE.\n"+
	"3. Warten Sie auf das 'Signal zur Abfahrt'.\n"+
	"TIPP: Verwenden Sie die Lokführerinformation 'Nächster Halt' (F10), um das Ein- und Aussteigen zu überwachen."
	)
    	Sound ( "talent_Cab.sms" )
)
