SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-START_80-76_204-2_Bpmbdfee
	Type ( Engine )
	WagonShape ( H-START_80-76_204-2_Bpmbdfee.s )
	Freightanim ( H-START_80-76_204-2_Bpmbdfee_kieg.s 1 1 )
	Size ( 2.883m 4.073m 26.2m )
	Mass ( 38t )
	WheelRadius ( 0.48m )
	InertiaTensor ( Box ( 2.883m 4.073m 26.2m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m  )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 2e7N 2e7N )
			r0 ( 0cm 1e9cm )
		)
		CouplingHasRigidConnection (  )
		Velocity ( 1m/s )
	)
	
	PassengerCapacity ( 30 )

	Inside (
                PassengerCabinFile      ( H-START_80-76_204-2_Bpmbdfee.s )
                PassengerCabinHeadPos ( 0.0 2.6 -8.5 )
                RotationLimit ( 360 360 360 )
                StartDirection ( 0 0 0 )
	Sound ( "ec_sound.sms" )
	)
	Buffers (
		Spring (
			Stiffness ( 1e8N/m 0N/m )
			Damping ( 1e8N/m/s 0N/m/s)
			r0 ( 0m 1e9 )
		)
		Centre ( 1 )
		Radius ( 2 )
		Angle ( 1deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 7cm )
	DerailRailForce ( 95kN )
	DerailBufferForce ( 361kN )
	NumWheels (	4 )
	Friction (
		642.6N/m/s		0.05		1mph		3.046N/m/s		1.803
		5.1N/rad/s		1		-1rad/s		0		1
	)

	BrakeEquipmentType( "Triple_Valve, Auxilary_reservoir, Emergency_brake_reservoir" )

	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 56.6kN )						

	EmergencyBrakeResMaxPressure( 50 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 5 )
	MaxApplicationRate( 9 )
	MaxAuxilaryChargingRate( 4 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 4 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )
	EmergencyResVolumeMultiplier( 1.15 )
	BrakeAirPressureGainInResForOnePoundFromPipe( 0.25 )

	Lights	( 15
		Light	(
			comment( Sphere of light dim )
			Type		( 1 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.75 )
			FadeOut	( 0.75 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( aaffffbb )
					Position ( 0.0 3 1 )
					Transition ( 0 )
					Radius ( 20.0 )
					Angle ( 20.0 )
					)
				)
			)
		Light	(
			comment( Sphere of light bright )
			Type( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.75 )
			FadeOut	( 0.75 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( 0.0 3 3 )
					Transition ( 0 )
					Radius ( 60.0 )
					Angle ( 15.0 )
					)
				)
			)
		Light	(
			comment( Head light top dim )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ffffbb )
					Position ( 0.0 3.6 12.48 )
					Azimuth ( 0 00 0 )
					Transition ( 1 )
					Radius ( 0.45 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Head light right dim )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ffffbb )
					Position ( -1.03 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.45 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Head light left dim )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ffffbb )
					Position ( 1.03 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.45 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Head light top bright )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( 0.0 3.6 12.48 )
					Azimuth ( 0 0 0 )
					Transition ( 1 )
					Radius ( 0.6 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Head light right bright )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( -1.03 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Head light left bright )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( 1.03 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Rear red light )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1

				State	(
					Duration ( 0 )
					LightColour ( 90ff0000 )
					Position ( -0.743 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.35 )
				)
			)
		)
		Light	(
			comment( Rear red light )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1

				State	(
					Duration ( 0 )
					LightColour ( 90ff0000 )
					Position ( 0.743 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.35 )
				)
			)
		)		
		
		Light	(
			comment( Service Head light top )
			Type( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( 0.0 3.6 12.48 )
					Azimuth ( 0.0 180.0 0.0 )
					Transition ( 1 )
					Radius ( 0.6 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Service Head light right ) 
			Type( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( -1.03 1.76 12.95 )
					Azimuth ( 0.0 180.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( Service Head light left )
			Type( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffbb )
					Position ( 1.03 1.76 12.95 )
					Azimuth ( 0.0 180.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
			Light	(
			comment( Service Rear red light )
			Type		( 0 )
			Conditions	(
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )

				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1

				State	(
					Duration ( 0 )
					LightColour ( 90ff0000 )
					Position ( -0.743 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.35 )
				)
			)
		)
		Light	(
			comment( Service Rear red light )
			Type		( 0 )
			Conditions	(
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1

				State	(
					Duration ( 0 )
					LightColour ( 90ff0000 )
					Position ( 0.743 1.76 12.95 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.35 )
				)
			)
		)		
	)
	Sound ( "H_Steuerwageng_478.sms" )
)

Engine ( H-START_80-76_204-2_Bpmbdfee
	Wagon ( H-START_80-76_204-2_Bpmbdfee )
	Name ( "H-START_80-76_204-2_Bpmbdfee" ) 
	Type ( Electric )
	MaxPower ( 6kW )
	MaxForce ( 0.1kN )
	MaxContinuousForce ( 0.1kN )
	MaxVelocity ( 160kmh )
	MaxCurrent ( 1640A )
	WheelRadius ( 0.48m )
	Sanding ( 6mph )
	NumWheels ( 1 ) 
	Sound ( "H_Steuerwagcab_478.sms" )
	CabView ( 8075.cvf )
	HeadOut ( 1.6 2.56 11.05 )
									
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )

	EngineBrakesControllerDirectControlExponent( 1 )

	BrakesEngineControllers( "Independent, Train" )			
	DoesBrakeCutPower( 1 )
	BrakeCutsPowerAtBrakeCylinderPressure( 5 )				

	AirBrakesAirCompressorPowerRating( 3 )
	AirBrakesMainMinResAirPressure( 72 )
	AirBrakesMainMaxAirPressure( 143 )
	AirBrakesMainResVolume( 25 )
	AirBrakesAirCompressorWattage( 30000 )
	AirBrakesCompressorRestartPressure( 107 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.9 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 10 )
	EngineBrakesControllerMaxReleaseRate( 10 )
	EngineBrakesControllerEmergencyApplicationRate( 15 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72.5 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 30 )

	TrainBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMaxApplicationRate( 9 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerEmergencyApplicationRate( 12 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerFullServicePressureDrop( 25 )

	DoesHornTriggerBell( 0 )

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 38 )
		MonitoringDeviceAlarmTimeLimit ( 30 )
		MonitoringDevicePenaltyTimeLimit ( 5 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 0 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		)
	
    EngineControllers (
            Throttle ( 0 1 0.05 0 
                NumNotches ( 0
                )
            )
            Brake_Engine ( 0 1 0.04 0
                NumNotches ( 3
                    Notch ( 0 0 EngineBrakesControllerReleaseStart ) 
                    Notch ( 0.1 1 EngineBrakesControllerGraduatedSelfLapLimitedHoldingStart ) 
                    Notch ( 0.95 0 EngineBrakesControllerFullServiceStart ) 
                )
            )
            Brake_Train ( 0 1 0.0125 0.28 
                NumNotches ( 5
                    Notch ( 0    0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.2  0 TrainBrakesControllerNeutralhandleOffStart )
                    Notch ( 0.25 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.75 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
                )
            )
            DirControl ( -1 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            EmergencyStopResetToggle( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1  ( 0 1 0)
            PantographToggle2  ( 0 1 0 )
            PantographsToggle_5  ( 0 1 2 ) 
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 ) 					
        )

        Description (
		"Ein moderner Bahnbetrieb bedingt auch ein schnelles Wenden der Zuege. Die OeBB begannen daher die nicht "+
		"mehr benoetigten Speisewagen der langen Schlieren Serie auf Steuerwagen fuer Wendezugbetrieb umzubauen. "+
		"Als Triebfahrzeug wurde auch die 1042 fuer Wendezugbetrieb mit einer dem entsprechenden Steuerung ausgestattet und auf 1142 umgereiht. "+
		"Zuerst waren die Steuerwagen im Verkehrsrot Grauweiss lackiert nun sind sie im Cityshuttle Design unterwegs. "
        )
        EngineOperatingProcedures (
        "So setzen Sie den Zug in Bewegung\n"+
        "1. Drücken Sie die P-TASTE, um den Stromabnehmer auszufahren.\n"+
	"2.	Drücken Sie die W-TASTE, um den Richtungshebel in die Position Vorwärts zu stellen.\n"+
	"3.	Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n"+
	"4. 	Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n"+
	"5.	Drücken Sie die D-TASTE, um die Reglereinstellung zu erhöhen.\n\n"+  
	"So bremsen Sie den Zug ab\n"+
	"1.	Drücken Sie die A-TASTE, um den Regler nach unten zu bewegen.\n"+
	"2.	Setzen Sie die Bremsen ein, wenn Sie noch weiter abbremsen möchten.\n\n"+
	"So bedienen Sie die Zugbremsen\n"+
	"1.	Drücken Sie die Ä-TASTE, um die Zugbremse zu ziehen.\n\n"+
	"So lösen Sie die Zugbremsen\n"+
	"1. Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n\n"+
	"So betätigen Sie die Lokbremse\n"+
	"1.	Drücken Sie die +-TASTE (Pluszeichen), um die Lokbremse anzuziehen.\n\n"+
		"So lösen Sie die Lokbremse\n"+
	"1. Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n\n"+
	"So lösen Sie die Notbremse aus\n"+
	"1.	Drücken Sie die A-TASTE, um den Regler in die Position Leerlauf zu stellen.\n"+
	"2.	Drücken Sie die RÜCKTASTE, um die Notbremsung auszulösen.\n\n"+
	"So fahren Sie rückwärts\n"+
	"1.	Halten Sie den Zug vollständig an.\n"+
	"2.	Drücken Sie die S-TASTE, um den Richtungshebel in die Position Rückwärts zu stellen.\n"+
	"3.	Drücken Sie die Ö-TASTE und die Ü-TASTE, um die Bremsen zu lösen.\n"+
	"4.	Schieben Sie den Regler langsam nach vorne (D-TASTE).\n\n"+
	"So lassen Sie Fahrgäste ein- und aussteigen\n"+
	"1. Halten Sie an einem Bahnhof an.\n"+
	"2. Drücken Sie die EINGABETASTE.\n"+
	"3. Warten Sie, bis das Signal die Erlaubnis zur Abfahrt gibt.\n"+
	"TIPP: Verwenden Sie die Lokführerinformation 'Nächster Halt' (F10), um das Ein- und Aussteigen zu überwachen.\n\n"
        ) 
	Name ( "H-START_80-76_204-2_Bpmbdfee" ) 
)

