SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( TH_400_865
	Type ( Engine )
	WagonShape ( TH_400_865.s )
 	Freightanim ( TH_400_865_freight.s 1 1 ) 
	Size ( 3.56m 4.83m 19.77m )  
	Mass ( 120t )
	WheelRadius ( 625mm )
	InertiaTensor ( Box ( 3.56m 4.83m 19.77m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 3e6N/m )
			Damping ( 9.9e5N/m/s 2.99e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 0.5cm 20cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 0.7e6N/m 0 )
			Damping ( 1e6N/m/s 0 )
			r0 ( 5cm 15cm )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 90deg )
	)
	Adheasion ( 0.19   0.76   1.5   0 )	
	DerailRailHeight ( 10cm )
	DerailRailForce ( 300kN )
	DerailBufferForce ( 800kN )
	NumWheels( 3 )
	Friction (
		1378.8N/m/s		-0.05		1.0mph		10.449N/m/s		1.863
		5.1N/rad/s		  1		-1rad/s			0			  1
	)

	
	BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir" )

	BrakeSystemType ( "Air_single_pipe" )
	MaxBrakeForce( 66kN )
	
	TripleValveRatio( 2.42 )
	MaxReleaseRate( 1.05 )
	MaxApplicationRate( 2.07 )
	MaxAuxilaryChargingRate( 0.2 )	
	BrakeCylinderPressureForMaxBrakeBrakeForce( 54 )

	Sound ( "LE1eng.sms" )

	Lights ( 26
  
  comment ( Capitolul 1 - Lumini pe linie )
  
  Light (
   comment( 1 Sfera luminoasa mare in fata )
   
   Type ( 1 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffffcc )
     Position ( 0.0 3.8 7.8 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 250.0 )
     Angle ( 12.0 )
    )
   )
  )
 
 Light (
   comment( 2 Sfera luminoasa mica in fata )
   
   Type ( 1 )
   Conditions (
    Headlight ( 2 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffffcc )
     Position ( 0.0 3.8 7.8 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 60.0 )
     Angle ( 15.0 )
    )
   )
 )
 
 comment ( Capitolul 2 - Faruri centrale )

 Light (
   comment( 3 Far central fata dreapta )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( 0.12 3.7 9.49 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
 Light (
   comment( 4 Far central fata dreapta AI )
   Type  ( 0 )
   Conditions (
 Control ( 1 )
 Unit ( 2 )
 Service ( 2 )
 TimeOfDay ( 2 )
 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( 0.12 3.7 9.49 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
 Light (
   comment( 5 Far central fata stanga )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( -0.12 3.7 9.49 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
 Light (
   comment( 6 Far central fata stanga AI )
   Type  ( 0 )
   Conditions (
 Control ( 1 )
 Unit ( 2 )
 Service ( 2 )
 TimeOfDay ( 2 )
 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( -0.12 3.7 9.49 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
 Light (
   comment( 7 Far central spate dreapta )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( 0.12 3.7 -9.49 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
   Light (
   comment( 8 Far central spate stanga )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 5 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( -0.12 3.7 -9.49 )
     Azimuth ( 180.0 180.0 180.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
  
  comment ( Capitolul 3 - Coltar dreapta fata )
  
  Light (
   comment( 9 Alb 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( 0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 10 Alb 3 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( 0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 11 Alb 5 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( 0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 12 Alb AI )
   Type  ( 0 )
   Conditions (
 Control ( 1 )
 Unit ( 2 )
 Service ( 2 )
 TimeOfDay ( 2 )
 )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( 0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 13 Rosu 4 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 4 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
 
 comment ( Capitolul 4 - Coltar stanga fata )

  Light (
   comment( 14 Alb 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( -0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 15 Alb 3 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( -0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 16 Alb 5 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( -0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 17 Alb AI )
   Type  ( 0 )
   Conditions (
 Control ( 1 )
 Unit ( 2 )
 Service ( 2 )
 TimeOfDay ( 2 )
 )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffe4ab )
     Position ( -0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 18 Rosu 4 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 4 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.875 1.87 9.7 )
     Azimuth ( 0.0 0.0 0.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )

 comment ( Capitolul 5 - Coltar dreapta spate )

  Light (
   comment( 19 Alb 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( 0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 20 Alb 4 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 4 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( 0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 21 Alb 5 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( 0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 22 Rosu 3 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )

comment ( Capitolul 6 - Coltar stanga spate )

  Light (
   comment( 23 Alb 2 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( -0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 24 Alb 4 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 4 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( -0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 25 Alb 5 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 5 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80eedf90 )
     Position ( -0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  Light (
   comment( 26 Rosu 3 )
   Type  ( 0 )
   Conditions (
    Headlight ( 4 )
    Unit ( 3 )
    )
   Cycle ( 0 )
   FadeIn ( 0.4 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( -0.875 1.87 -9.7 )
     Azimuth ( -180.0 -180.0 -180.0 )
     Transition ( 0 )
     Radius ( 0.3 )
     )
    )
   )
  )
 )
	
Engine ( TH_400_865
	Wagon ( TH_400_865 )
	Type ( Electric )
	MaxPower ( 5100kW )
	MaxForce ( 421kN )
	MaxContinuousForce ( 367.63kN )
	MaxVelocity ( 120km/h )
	MaxCurrent ( 1700A )
	WheelRadius ( 625mm )
	Sanding ( 5 km/h )
	NumWheels( 3 )

	CabView ( LE_CL.cvf )
	HeadOut ( 1.75 3.1 8.2 )

	AirBrakeMaxMainResPipePressure( 145 )
	AirBrakesAirCompressorPowerRating( 2.25 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 145 )
	AirBrakesMainResVolume( 26.19 )
	AirBrakesAirCompressorWattage( 44000 )
	AirBrakesCompressorRestartPressure( 116 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2.25 )
	AirBrakesHasLowPressureTest( 0 )
	AirBrakesIsCompressorElectricOrMechanical( 0 )

	EngineBrakesControllerMinPressureReduction( 2.25 )
	TrainBrakesControllerMinPressureReduction( 2.25 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 1.5 )
	TrainBrakesControllerMaxApplicationRate( 1.5 )
	EngineBrakesControllerMaxReleaseRate( 1.5 )
	TrainBrakesControllerMaxReleaseRate( 1.5 )
	EngineBrakesControllerMaxQuickReleaseRate( 15 )
	TrainBrakesControllerMaxQuickReleaseRate( 15 )
	EngineBrakesControllerEmergencyApplicationRate( 1.49 )
	TrainBrakesControllerEmergencyApplicationRate( 1.49 )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72 ) 
	TrainBrakesControllerMaxSystemPressure( 72 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 21.75 )
	TrainBrakesControllerFullServicePressureDrop( 21.75 )

	DynamicBrakesMinUsableSpeed( 20 )
	DynamicBrakesMaximumEffectiveSpeed( 75 )
	DynamicBrakesMaximumForce( 200kN  )
	DynamicBrakesResistorCurrentLimit ( 850 )
	DynamicBrakesCutInSpeed( 5 )
	DynamicBrakesMaxAirBrakePressure ( 54 )
	DynamicBrakesFadingSpeed( 17 )
	DynamicBrakesDelayTimeBeforeEngaging ( 5 )
	DynamicBrakesMaximumSpeedForFadeOut ( 80 )
	DynamicBrakesEffectAtMaximumFadeOut( 0.34 )
	DynamicBrakesHigherSpeedCurveExponent( 1.2 )
	DynamicBrakesLowerSpeedCurveExponent( 0.9 )
	DynamicBrakesNumberOfControllerNotches( 40 )
	DynamicBrakeHasAutoBailOff( 0 )

      BrakesEngineBrakeType ( "Air_single_pipe"  )
	BrakesTrainBrakeType ( "Air_single_pipe" )
      BrakesEngineControllers( "Independent, Train, Dynamic" )
        
      EngineBrakesControllerDirectControlExponent( 1 )
		
	EmergencyStopMonitor(
   		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 45 )
		MonitoringDeviceAlarmTimeLimit( 37 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		)
		
        EngineControllers (
	      Throttle ( 0 1 0.025 0 
                NumNotches ( 41
                    Notch ( 0       0 Dummy )
                    Notch ( 0.025   0 Dummy )
                    Notch ( 0.05    0 Dummy )
                    Notch ( 0.075   0 Dummy )
                    Notch ( 0.1     0 Dummy )
                    Notch ( 0.125   0 Dummy )
                    Notch ( 0.15    0 Dummy )
                    Notch ( 0.175   0 Dummy )
                    Notch ( 0.2     0 Dummy )
                    Notch ( 0.225   0 Dummy )
                    Notch ( 0.25    0 Dummy )
                    Notch ( 0.275   0 Dummy )
                    Notch ( 0.3     0 Dummy )
                    Notch ( 0.325   0 Dummy )
                    Notch ( 0.35    0 Dummy )
                    Notch ( 0.375   0 Dummy )
                    Notch ( 0.4     0 Dummy )
                    Notch ( 0.425   0 Dummy )
                    Notch ( 0.45    0 Dummy )
                    Notch ( 0.475   0 Dummy )
                    Notch ( 0.5     0 Dummy )
                    Notch ( 0.525   0 Dummy )
                    Notch ( 0.55    0 Dummy )
                    Notch ( 0.575   0 Dummy )
                    Notch ( 0.6     0 Dummy )
                    Notch ( 0.625   0 Dummy )
                    Notch ( 0.65    0 Dummy )
                    Notch ( 0.675   0 Dummy )
                    Notch ( 0.7     0 Dummy )
                    Notch ( 0.725   0 Dummy )
                    Notch ( 0.75    0 Dummy )
                    Notch ( 0.775   0 Dummy )
                    Notch ( 0.8     0 Dummy )
                    Notch ( 0.825   0 Dummy )
                    Notch ( 0.85    0 Dummy )
                    Notch ( 0.875   0 Dummy )
                    Notch ( 0.9     0 Dummy )
                    Notch ( 0.925   0 Dummy )
                    Notch ( 0.95    0 Dummy )
                    Notch ( 0.975   0 Dummy )
                    Notch ( 1       0 Dummy )
			)
            )
           Brake_Engine ( 0 1 0.0125 0
                NumNotches ( 3
                    Notch(0     1 EngineBrakesControllerReleaseStart )
                    Notch(0.05  1 EngineBrakesControllerHoldStart )
                    Notch(0.15  1 EngineBrakesControllerApplyStart )                    
                )
            )
            Brake_Train ( 0 1 0.075 0.65
                  NumNotches ( 6
                    Notch ( 0    0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch ( 0.1  0 TrainBrakesControllerReleaseStart )
                    Notch ( 0.2  0 TrainBrakesControllerNeutralhandleOffStart )		 
                    Notch ( 0.3  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
		        Notch ( 0.9  0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 1.0  0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Dynamic ( 0 1 0.025 0 
                NumNotches ( 41 
                    Notch ( 0       0 Dummy )
                    Notch ( 0.025   0 Dummy )
                    Notch ( 0.05    0 Dummy )
                    Notch ( 0.075   0 Dummy )
                    Notch ( 0.1     0 Dummy )
                    Notch ( 0.125   0 Dummy )
                    Notch ( 0.15    0 Dummy )
                    Notch ( 0.175   0 Dummy )
                    Notch ( 0.2     0 Dummy )
                    Notch ( 0.225   0 Dummy )
                    Notch ( 0.25    0 Dummy )
                    Notch ( 0.275   0 Dummy )
                    Notch ( 0.3     0 Dummy )
                    Notch ( 0.325   0 Dummy )
                    Notch ( 0.35    0 Dummy )
                    Notch ( 0.375   0 Dummy )
                    Notch ( 0.4     0 Dummy )
                    Notch ( 0.425   0 Dummy )
                    Notch ( 0.45    0 Dummy )
                    Notch ( 0.475   0 Dummy )
                    Notch ( 0.5     0 Dummy )
                    Notch ( 0.525   0 Dummy )
                    Notch ( 0.55    0 Dummy )
                    Notch ( 0.575   0 Dummy )
                    Notch ( 0.6     0 Dummy )
                    Notch ( 0.625   0 Dummy )
                    Notch ( 0.65    0 Dummy )
                    Notch ( 0.675   0 Dummy )
                    Notch ( 0.7     0 Dummy )
                    Notch ( 0.725   0 Dummy )
                    Notch ( 0.75    0 Dummy )
                    Notch ( 0.775   0 Dummy )
                    Notch ( 0.8     0 Dummy )
                    Notch ( 0.825   0 Dummy )
                    Notch ( 0.85    0 Dummy )
                    Notch ( 0.875   0 Dummy )
                    Notch ( 0.9     0 Dummy )
                    Notch ( 0.925   0 Dummy )
                    Notch ( 0.95    0 Dummy )
                    Notch ( 0.975   0 Dummy )
                    Notch ( 1       0 Dummy )
                )
            )
            
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
     	      Combined_Control( 0 1 0.5 0.5 throttle dynamic )
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
	      EmergencyStopResetToggle( 0 1 0 )
            PantographToggle1  ( 0 1 0 )
	      PantographToggle2  ( 0 1 0 )	
            Wipers ( 0 -1 0 )
	      BailOffButton( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
        )

 	Sound ( "LE1cab.sms" )
 	Name ( "TRAIN HUNGARY 400 865-8" )
 	        Description (
	"Locomotiva electrica LE5100 3.0
         -Construirea lor a inceput in 1965 in Suedia unde s-au facut primele 10 locomotive sub licenta ASEA,pana in anul 1991 s-au facut peste 1000 de locomotive.
         Formula osiilor:- Co-Co
         Diametrul rotilor:-1250mm
         Greutate:-120t
         Lungime:-19800mm
         Latime:-3000mm
         Inaltime:-4620mm(cu pantograful coborat)
         Tensiune de alimentare:-27000V
         Frecventa de alimentare:-50Hz
         Putere:-5100kw ( 6839 hp )

        -Modelul 3D Realizat de: Csiszer Istvan (Balkanrail)
)
	EngineOperatingProcedures (
    "To move forward\n"+
    "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
    "2.	Press the W key to move the Reverser to Forward.\n"+
    "3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
    "4.	Press the D key to move increase the throttle setting.\n\n"+  
    "To slow the train\n"+
    "1.	Press the A key to move the throttle to a lower setting.\n"+
    "2.	Use the brakes to further reduce speed if desired.\n\n"+   
    "To apply the train brakes\n"+
    "1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
    "To release the train brakes\n"+
    "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
    "To activate emergency braking\n"+
    "1.	Press the A key to reduce the throttle to Idle.\n"+
    "2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
    "To back up\n"+
    "1.	Bring your train to a full stop.\n"+
    "2.	Press the S key to move the Reverser to the Reverse position.\n"+
    "3.	Press the ; (SEMICOLON)  to release the brakes.\n"+
    "4.	Slowly advance the throttle lever (D key).\n\n"+
    "To load and unload passengers\n"+
    "1. Stop at a station.\n"+
    "2. Press the ENTER key.\n"+
    "3. Wait for the 'permission to depart' signal.\n"+
    "TIP: Use the Next Station driving aid (F10) to monitor loading and unloading."
	)
)
