SIMISA@@@@@@@@@@JINX0D0t______

        Wagon ( 185-608-7
	Type ( Engine )
	WagonShape ( 185-608-7.s )
	FreightAnim ( 185-608-7_fa.s 1 1 )
	Size ( 3.1m 4.558m 18.9m )
	Mass ( 82t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.1m 4.558m 18.9m ))
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 3e9N 3e9N )
			r0 ( 0cm 1e9 )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 200KN )
	DerailBufferForce ( 1000kN )
	NumWheels ( 0 )
	Friction (
		1054N/m/s		0	 1mph		   1.60N/m/s	1.8
		5.1N/rad/s		1	-1rad/s	   	   0		1
	)
	AntiSlip ()

	BrakeEquipmentType( "graduated_release_triple_valve , Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 84kN )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 40 )
	MaxApplicationRate( 30 )
	MaxAuxilaryChargingRate( 116 )
	EmergencyResCapacity( 25 )
	EmergencyResChargingRate( 25 )
	EmergencyBrakeResMaxPressure( 70 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	Sound ( "145_Eng.sms" )

	Lights ( 29
		Light (
			comment ( Lichtkegel #1 )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0 1.4 6.5 )
					Angle ( 20 )
					Transition ( 0 )
					Radius ( 45 )
				)
			)
		)
		Light (
			comment ( Lichtkegel #2 )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFCC )
					Position ( 0.02 1.4 6.5 )
					Angle ( 20 )
					Transition ( 0 )
					Radius ( 60 )
				)
			)
		)
		Light (
			comment ( vorn mitte abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0 2.45 8.9 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( vorn mitte aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0 2.45 8.9 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( vorn rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( -0.66 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( vorn links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0.66 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( vorn rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( -0.88 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( vorn links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( 0.88 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( hinten rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.88 1.65 -9.025 )
					Azimuth ( 180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( hinten links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.88 1.65 -9.025 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( hinten rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.88 1.65 -9.025 )
					Azimuth ( 180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( hinten links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.88 1.65 -9.025 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe mitte abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0 2.45 -8.9 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe mitte aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0 2.45 -8.9 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( -0.66 1.65 -9.025 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0.66 1.65 -9.025 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0.88 1.65 -9.025 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0.88 1.65 -9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( -0.88 1.65 -9.025 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_twin_pipe links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFFF )
					Position ( 0.88 1.65 -9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_single_pipe rechts abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.88 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_single_pipe links abgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.88 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_single_pipe rechts aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.88 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( Vacuum_single_pipe links aufgeblendet )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.88 1.65 9.025 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( AI vorn mitte  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				Coupling ( 0 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0 2.45 8.9 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( AI vorn rechts  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				Coupling ( 0 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( -0.88 1.65 9.025 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( AI vorn links  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				Coupling ( 0 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFFFBB )
					Position ( 0.88 1.65 9.025 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( AI hinten rechts  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				Coupling ( 0 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.88 1.65 -9.025 )
					Azimuth ( 180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
		Light (
			comment ( AI hinten links  )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				Weather ( 0 )
				Coupling ( 0 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.88 1.65 -9.025 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
				)
			)
		)
	)
)

        Engine ( 185-608-7
	Wagon ( 185-608-7 )
	Type ( Electric )
	MaxPower ( 5600kW )
	MaxForce ( 300kN )
	MaxContinuousForce ( 300kN )
	MaxVelocity ( 160kmh )
	MaxCurrent ( 1640A )
	WheelRadius ( 0.5m )
	Sanding ( 20kmh )
	NumWheels ( 1 )

	CabView ( "tser480002.cvf" )
        HeadOut ( 1.7 2.9 7.4 )

	AirBrakesAirCompressorPowerRating ( 300 )
	AirBrakesAirCompressorWattage ( 30000 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 0.1 )
	AirBrakesCompressorRestartPressure ( 135 )
	AirBrakesIsCompressorElectricOrMechanical ( 1 )
	AirBrakesMainMaxAirPressure ( 140 )
	AirBrakesMainMinResAirPressure ( 0 )
	AirBrakesMainResVolume ( 30 )

	EngineBrakesControllerMinPressureReduction ( 6 )
	EngineBrakesControllerMaxApplicationRate ( 30 )
	EngineBrakesControllerMaxReleaseRate ( 40 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 110 )
            EngineBrakesControllerEmergencyApplicationRate ( 50 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	EngineBrakesControllerFullServicePressureDrop ( 50 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerDirectControlExponent ( 1 )
            EngineBrakesProportionalBrakeLag( 0.1 )
               
	TrainBrakesControllerMinPressureReduction ( 5 )
	TrainBrakesControllerMaxApplicationRate ( 30 )
	TrainBrakesControllerMaxReleaseRate ( 40 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 110 )
	TrainBrakesControllerMaxQuickReleaseRate ( 80 )
            TrainBrakesControllerEmergencyApplicationRate ( 50 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	TrainBrakesControllerFullServicePressureDrop ( 50 )

   	DynamicBrakesMinUsableSpeed( 0 )
   	DynamicBrakesMaximumEffectiveSpeed( 0 )
    	DynamicBrakesMaximumForce( 150KN )
    	DynamicBrakesResistorCurrentLimit ( 5000 )
    	DynamicBrakesCutInSpeed( -110 )
    	DynamicBrakesMaxAirBrakePressure ( 50 )
    	DynamicBrakesFadingSpeed( 110 )
    	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
    	DynamicBrakesMaximumSpeedForFadeOut ( 110 )
    	DynamicBrakesEffectAtMaximumFadeOut( 0 )
    	DynamicBrakesHigherSpeedCurveExponent( 1 )
    	DynamicBrakesLowerSpeedCurveExponent( 1 )
    	DynamicBrakesNumberOfControllerNotches( 0 )

	BrakesEngineBrakeType ( Air_single_pipe )
	BrakesTrainBrakeType ( Air_single_pipe )
	BrakesEngineControllers( "Independent, Train, Dynamic" )

	BrakeCutsPowerAtBrakeCylinderPressure ( 15 )

	DoesBrakeCutPower ( 1 )
	DoesHornTriggerBell ( 0 )

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 55 )
		MonitoringDeviceAlarmTimeLimit ( 40 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 100 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 100 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 104 )
		MonitoringDeviceResetLevel ( 104 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceResetOnResetButton ( 1 )
		MonitoringDeviceResetOnZeroSpeed ( 0 )
		)
               EngineControllers (
                 Throttle ( 0 1 0.025 0
                            NumNotches ( 0
			)
		)
	Brake_Engine ( 0 1 0.04 0
		NumNotches ( 1
			Notch ( 0 1 Dummy )
			)
		)
	Brake_Train ( 0 1 0.03 0.33
		NumNotches ( 5
		Notch ( 0      0 TrainBrakesControllerReleaseStart )
		Notch ( 0.3   1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
		Notch ( 0.85 0 TrainBrakesControllerSuppressionStart )
		Notch ( 0.9   0 TrainBrakesControllerContinuousServiceStart )
		Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
		)
	)
	Brake_Dynamic ( 0 1 0.05 0
		NumNotches ( 1
			Notch ( 0 1 Dummy )
		)
	)
	DirControl ( -1 0 1 1 )
	EmergencyStopToggle ( 0 1 0 )
	EmergencyStopResetToggle ( 0 1 0 )
	PantographToggle1 ( 0 1 0 )
	PantographToggle2 ( 0 1 0 )
	Headlights ( 0 0.25 1 0 )
	Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
	Sanding ( 0 1 0 )
	BellToggle ( 0 1 0 )
	Vigilance ( 0 1 0 )
	)
	Sound ( "145_Cab.sms" )
	Name ( "185-608-7" )
	Description (
       	"Technische Daten:\n"+
	"Lokomotivtyp: Elektrische Drehstromlokomotive\n"+
	"Leistung: 5.600 Kw\n"+
	"Vmax: 160 km/h \n"+
	"Betriebsmasse: 82t\n"+
	"Max. temporäre Zugkraft: 300kN \n"+
	"Achsfolge: Bo'Bo'" )
        EngineOperatingProcedures (
        "So setzen Sie den Zug in Bewegung\n"+
        "1. Der Stromabnehmer wurde bereits ausgefahren. (Sollte dies aus irgendeinem Grund noch nicht geschehen sein, drücken Sie die P-TASTE, um den Stromabnehmer auszufahren.)\n"+
	"2.	Drücken Sie die W-TASTE, um den Richtungshebel in die Position Vorwärts zu stellen.\n"+
	"3.	Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n"+
	"4. 	Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n"+
	"5.	Drücken Sie die D-TASTE, um die Reglereinstellung zu erhöhen.\n\n"+  
	"So bremsen Sie den Zug ab\n"+
	"1.	Drücken Sie die A-TASTE, um den Regler nach unten zu bewegen.\n"+
	"2.	Setzen Sie die Bremsen ein, wenn Sie noch weiter abbremsen möchten.\n\n"+
	"So bedienen Sie die Zugbremsen\n"+
	"1.	Drücken Sie die Ä-TASTE, um die Zugbremse zu ziehen.\n\n"+
	"So lösen Sie die Zugbremsen\n"+
	"1. Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n\n"+
	"So lösen Sie die Zugbremsen auf der Lokomotive getrennt\n"+
	"1. Drücken Sie --TASTE (MINUS).\n\n"+
	"So betätigen Sie die Lokbremse\n"+
	"1.	Drücken Sie die +-TASTE (Pluszeichen), um die Lokbremse anzuziehen.\n\n"+
		"So lösen Sie die Lokbremse\n"+
	"1. Drücken Sie die Ü-TASTE, um die Lokbremse zu lösen.\n\n"+
	"So lösen Sie die Notbremse aus\n"+
	"1.	Drücken Sie die A-TASTE, um den Regler in die Position Leerlauf zu stellen.\n"+
	"2.	Drücken Sie die RÜCKTASTE, um die Notbremsung auszulösen.\n\n"+
	"So fahren Sie rückwärts\n"+
	"1.	Halten Sie den Zug vollständig an.\n"+
	"2.	Drücken Sie die S-TASTE, um den Richtungshebel in die Position Rückwärts zu stellen.\n"+
	"3.	Drücken Sie die Ö-TASTE und die Ü-TASTE, um die Bremsen zu lösen.\n"+
	"4.	Schieben Sie den Regler langsam nach vorne (D-TASTE).\n\n"+
	"So lassen Sie Fahrgäste ein- und aussteigen\n"+
	"1. Halten Sie an einem Bahnhof an.\n"+
	"2. Drücken Sie die EINGABETASTE.\n"+
	"3. Warten Sie, bis das Signal die Erlaubnis zur Abfahrt gibt.\n"+
	"TIPP: Verwenden Sie die Lokführerinformation 'Nächster Halt' (F10), um das Ein- und Aussteigen zu überwachen.\n\n"+
	"So kuppeln Sie an einen Waggon oder eine Lokomotive an\n"+
	"1. Fahren Sie sehr langsam an die Einheit heran, mit etwa 2 km/h.\n"+
	"TIPP: Drücken Sie die 6-TASTE, um in die Kupplungsansicht zu wechseln.\n"+
	"2. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n"+
	"3. Wenn das Symbol für die angekuppelte Einheit rot angezeigt wird, ist die Handbremse gezogen. Doppelklicken Sie auf den Waggon, um die Handbremse zu lösen.\n"+
	"4. Schließen Sie das Zugbedienungsfenster.\n\n"+
	"So kuppeln Sie von einem Waggon oder einer Lokomotive ab\n"+
	"1. Drücken Sie F9, um das Zugbedienungsfenster zu öffnen.\n"+
	"2. Doppelklicken Sie auf eine Einheit in dem Bereich des Zuges, den Sie von der Lokomotive abkuppeln möchten, um die Handbremse zu ziehen.\n"+
	"3. Doppelklicken Sie auf die Kupplung zwischen den Einheiten, die Sie vom Rest des Zuges abkuppeln möchten.\n"+
	"4. Schließen Sie das Fenster Zugbedienung."
        )
)
