SIMISA@@@@@@@@@@JINX0D0t______
 
Wagon ( mav_470.007
 Type ( Engine ) 
 WagonShape ( mav_470.007.s ) 
 Freightanim ( mav_470.007_freight.s 1 1 ) 
 
Comment ( Verze ladeni ENG : bob57_cz , 10.9.2011 )
Comment ( Nastaveni svetel : David Hajek ) 
 
 Size  ( 2.96m 4.445m 19.28m )
 CentreOfGravity ( 0m 2.25m 0m ) 
 Mass ( 85t ) 
 WheelRadius ( 0.625m ) 
 InertiaTensor ( Box ( 2.9m 4.4m 19.2m ) ) 
 
 Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 1cm 25cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
 
 Adheasion ( 0.60 0.78 1.8 0 ) 
 DerailRailHeight ( 10cm ) 
 DerailRailForce ( 2.5*85t ) 
 DerailBufferForce ( 350kN ) 
 NumWheels ( 4 ) 
 
 Friction ( 800N/m/s  0.05  1mph  6.2N/m/s  1.1  4.1N/rad/s  1  0.1rad/s  0.1N/rad/s  1 ) 
 
 BrakeEquipmentType ( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" ) 
 BrakeSystemType ( "Air_single_pipe" ) 
 MaxBrakeForce ( 100kN ) 
 MaxHandbrakeForce ( 25kN ) 
 NumberOfHandbrakeLeverSteps ( 100 ) 
 BrakeCylinderPressureForMaxBrakeBrakeForce ( 56 ) 
 EmergencyBrakeResMaxPressure ( 72 ) 
 TripleValveRatio ( 2.92 ) 
 MaxReleaseRate ( 4.5 ) 
 MaxApplicationRate ( 2 ) 
 MaxAuxilaryChargingRate ( 2 ) 
 EmergencyResChargingRate ( 2 ) 
 EmergencyResVolumeMultiplier ( 2 ) 
 EmergencyResCapacity ( 0.3 ) 
 
 Lights ( 37 
 
Comment ( svetelne kuzely ) 

 Light ( comment ( 1 svetelny kuzel obrysove ) 
  Type ( 1 ) 
  Conditions ( 
  Headlight ( 1 ) 
  Unit ( 2 ) 
  Control ( 2 ) 
  TimeOfDay ( 2 ) 
  ) 
  FadeIn ( 0.1 ) 
  FadeOut ( 0.1 ) 
  Cycle ( 0 ) 
  States ( 1 
  State ( 
   Duration ( 0 ) 
   LightColour ( 16161616  ) 
   Position ( 0.0 1.7 -5 ) 
   Transition ( 0 )
   Angle ( 10 ) 
   Radius ( 20 ) 
 ) ) ) 
 
 Light ( Comment ( 2 Svetelny kuzel tlumeny ) 
  Type ( 1 ) 
  Conditions ( 
  Headlight ( 2 ) 
  Unit ( 2 ) 
  Control ( 2 ) 
  TimeOfDay ( 2 ) 
  ) 
  FadeIn ( 0.1 ) 
  FadeOut ( 0.1 ) 
  Cycle ( 0 ) 
  States ( 1 
  State ( 
   Duration ( 0 ) 
   LightColour ( 8b80734b ) 
   Position ( 0 3.5 5.2 ) 
   Transition ( 0 )
   Angle ( 10 ) 
   Radius ( 250 ) 
 ) ) ) 
 
 Light ( Comment ( 3 Svetelny kuzel dalkovy ) 
  Type ( 1 ) 
  Conditions ( 
  Headlight ( 3 ) 
  Unit ( 2 ) 
  Control ( 2 ) 
  ) 
  FadeIn ( 0.1 ) 
  FadeOut ( 0.1 ) 
  Cycle ( 0 ) 
  States ( 1 
  State ( 
   Duration ( 0 ) 
   LightColour ( fcf0e68c ) 
   Position ( 0 3.5 5.2 ) 
   Transition ( 0 )
   Angle ( 10 ) 
   Radius ( 250 ) 
 ) ) ) 

Comment ( Definice svetel pro predni stanoviste v cele vlaku )

		Light (
			Comment ( Predni reflektor dalkovy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 8.86 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni reflektor pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 8.86 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni reflektor pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 8.86 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.7 8.95 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.7 8.95 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.9 8.9 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.9 8.9 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.9 8.9 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.9 8.9 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni reflektor pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 -8.84 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.7 -8.95 )
					Azimuth ( -180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.7 -8.95 )
					Azimuth ( -180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
Comment ( Definice svetel pro predni stanoviste na postrku )

		Light (
			Comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( 1.04 1.7 -8.95 )
					Azimuth ( -180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( -1.04 1.7 -8.95 )
					Azimuth ( -180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

Comment ( Definice svetel pro zadni stanoviste v cele vlaku )
		
		Light (
			Comment ( Reflektor dalkovy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
				Service( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 1.0 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 -8.86 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Reflektor pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 -8.86 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.9 -8.9 )
					Azimuth ( 180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.9 -8.9 )
					Azimuth ( 180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.9 -8.9 )
					Azimuth ( 180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.9 -8.9 )
					Azimuth ( 180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.7 -8.95 )
					Azimuth ( 0 -30 -15 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 5 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.7 -8.95 )
					Azimuth ( 0 15 30 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
Comment ( Definice svetel pro zadni stanoviste na postrku )
		
		Light (
			Comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( 1.04 1.7 8.95 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light ( 
			Comment ( Zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( -1.04 1.7 8.95 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

Comment ( Definice svetel pro loko ovladanou PC v normalnim smeru )

		Light (
			Comment ( PC predni prave v cele soupravy normalni smer )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.7 8.95 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
		Light (
			Comment ( PC predni leve v cele soupravy normalni smer )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.7 8.95 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( PC koncove prave na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.7 -8.95 )
					Azimuth ( -180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 20 )
				)
			)
		)
		
		Light (
			comment ( PC pozicni leve na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.7 -8.95 )
					Azimuth ( -180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
Comment ( Definice svetel pro Loose consist )

		Light (
			Comment ( Reflektor pozicni - Loose consist )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Service ( 0 )
				Control ( 1 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 8.84 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light	(
			Comment( Predni prave pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.7 8.95 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
		Light	(
			Comment( Predni leve pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.7 8.95 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni reflektor pozicni - Loose consist )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Service ( 0 )
				Control ( 1 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 2.63 -8.84 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light	(
			Comment( Zadni prave pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.04 1.7 -8.95 )
					Azimuth ( -180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 20 )
				)
			)
		)

		Light	(
			Comment( Zadni leve pozicni - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.04 1.7 -8.95 )
					Azimuth ( -180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.30 )
					Elevation ( -20 -20 -20 )

					)
			)
		)
	) 
 Sound ( "..//..//common.snd//sndElok//es64u2eng.sms" ) 
 ) 
 
Engine ( mav_470.007
 Wagon ( mav_470.007 ) 
 Type ( Electric ) 
 Name ( "H-MAVTR 470 007-0" ) 
 MaxPower ( 6400kW ) 
 MaxForce ( 300kN ) 
 MaxContinuousForce ( 300kN ) 
 MaxCurrent ( 1200A ) 
 MaxVelocity ( 253km/h ) 
 DieselEngineSpeedOfMaxTractiveEffort ( 88km/h ) 
 WheelRadius ( 0.625m ) 
 Sanding ( 200km/h ) 
 NumWheels ( 4 ) 
 Sound ( "..//..//common.snd//sndElok//es64u2_MIREL_cab.sms" ) 
 CabView ( "..//..//common.cab//CABVIEW//470.cvf" )
 HeadOut ( 1.7 2.9 7.5 ) 
 
 AirBrakesAirCompressorPowerRating ( 1.2 ) 
 AirBrakesAirCompressorWattage ( 16000 ) 
 AirBrakesMainResVolume ( 40 ) 
 AirBrakesMainMaxAirPressure ( 145 ) 
 AirBrakesCompressorRestartPressure ( 116 ) 
 AirBrakesMainMinResAirPressure ( 73 ) 
 AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 ) 
 AirBrakesHasLowPressureTest ( 1 ) 
 AirBrakesIsCompressorElectricOrMechanical ( 0 ) 
 
 BrakesEngineControllers ( "Dynamic, Independent, Train" ) 
 BrakesEngineBrakeType ( "Air_single_pipe" ) 
 BrakesTrainBrakeType ( "Air_single_pipe" ) 
 
 DoesBrakeCutPower ( 1 ) 
 
 EngineBrakesControllerHasProportionalBrake ( 1 ) 
 EngineBrakesControllerMaxReleaseRate ( 5 ) 
 EngineBrakesControllerMaxApplicationRate ( 5 ) 
 EngineBrakesControllerEmergencyApplicationRate ( 10 ) 
 EngineBrakesControllerMinSystemPressure ( 0 ) 
 EngineBrakesControllerMaxSystemPressure ( 73 ) 
 EngineBrakesControllerFullServicePressureDrop ( 73 ) 
 EngineBrakesControllerDirectControlExponent ( 1 ) 
 EngineBrakesProportionalBrakeLag ( 0.8 ) 
 
 TrainBrakesControllerMaxQuickReleaseRate ( 6 ) 
 TrainBrakesControllerMaxReleaseRate ( 6 ) 
 TrainBrakesControllerMaxApplicationRate ( 6 ) 
 TrainBrakesControllerEmergencyApplicationRate ( 10 ) 
 comment(TrainBrakesControllerMinPressureReduction ( 3 ) )
 TrainBrakesControllerFullServicePressureDrop ( 23.2 ) 
 TrainBrakesControllerMinSystemPressure ( 0 ) 
 TrainBrakesControllerMaxSystemPressure ( 72.5 ) 
 TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
 TrainPipeLeakRate ( 0.033 )  
 
 DynamicBrakesResistorCurrentLimit ( 1200 ) 
 DynamicBrakesDelayTimeBeforeEngaging ( 0 ) 
 DynamicBrakesNumberOfControllerNotches ( 10 ) 
 DynamicBrakesMaxAirBrakePressure ( 55 ) 
 DynamicBrakeHasAutoBailOff ( 0 ) 
 DynamicBrakesMaximumForce ( 150kN ) 
 DynamicBrakesHigherSpeedCurveExponent ( 2 ) 
 DynamicBrakesLowerSpeedCurveExponent ( 2 ) 
 DynamicBrakesMaximumSpeedForFadeOut ( 430 ) 
 DynamicBrakesMaximumEffectiveSpeed ( 97 ) 
 DynamicBrakesFadingSpeed ( 9 ) 
 DynamicBrakesMinUsableSpeed ( 2 ) 
 DynamicBrakesCutInSpeed ( 1 ) 
 DynamicBrakesCutOutSpeed ( 1 ) 
 DynamicBrakesEffectAtMaximumFadeOut ( 1 )  
 
 OverspeedMonitor ( 
  MonitoringDeviceMonitorTimeLimit ( 0 ) 
  MonitoringDeviceAlarmTimeLimit ( 5 ) 
  MonitoringDevicePenaltyTimeLimit ( 0 ) 
  MonitoringDeviceCriticalLevel ( 0 ) 
  MonitoringDeviceResetLevel ( 0 ) 
  MonitoringDeviceTriggerOnHighCurrent ( 1250 ) 
  MonitoringDeviceAppliesFullBrake ( 0 ) 
  MonitoringDeviceAppliesEmergencyBrake ( 0 ) 
  MonitoringDeviceAppliesCutsPower ( 1 ) 
  MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 ) 
  MonitoringDeviceDoesSuppressionReset ( 0 ) 
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnDirectionNeutral ( 1 ) 
 ) 
 VigilanceMonitor ( 
  MonitoringDeviceMonitorTimeLimit ( 27 ) 
  MonitoringDeviceAlarmTimeLimit ( 17 ) 
  MonitoringDevicePenaltyTimeLimit ( 0 ) 
  MonitoringDeviceCriticalLevel ( 0 ) 
  MonitoringDeviceResetLevel ( 0 ) 
  MonitoringDeviceAppliesFullBrake ( 0 ) 
  MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
  MonitoringDeviceAppliesCutsPower ( 1 ) 
  MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 1 ) 
 ) 
EmergencyStopMonitor ( 
  MonitoringDeviceMonitorTimeLimit ( 0 ) 
  MonitoringDeviceAlarmTimeLimit ( 0 ) 
  MonitoringDevicePenaltyTimeLimit ( 0 ) 
  MonitoringDeviceCriticalLevel ( 0 ) 
  MonitoringDeviceResetLevel ( 0 ) 
  MonitoringDeviceAppliesFullBrake ( 1 ) 
  MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
  MonitoringDeviceAppliesCutsPower ( 1 ) 
  MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 1 ) 
  ) 
		 
EngineControllers ( 
 
 Throttle ( 0 1 0.05 0 
 NumNotches ( 1 
 Notch ( 0 1 Dummy ) 
 ) ) 
 
 Brake_Dynamic ( 0 1 0.1 0 
			NumNotches ( 0 )
            )
 
 Brake_Engine ( 0 1 0.1 0 
 NumNotches ( 1 
 Notch ( 0 1 Dummy ) 
 ) ) 
 
 Brake_Train ( 0 1 0.1 0.2 
 NumNotches ( 6 
 Notch ( 0.0 0 TrainBrakesControllerFullQuickReleaseStart ) 
 Notch ( 0.1 0 TrainBrakesControllerReleaseStart ) 
 Notch ( 0.2 0 TrainBrakesControllerNeutralhandleOffStart ) 
 Notch ( 0.3 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart ) 
 Notch ( 0.9 0 TrainBrakesControllerSuppressionStart ) 
 Notch ( 1.0 0 TrainBrakesControllerEmergencyStart ) 
 ) ) 
 
 AWS ( 0 1 0 ) 
 BailOffButton ( 0 1 0 ) 
 BellToggle ( 0 1 0 ) 
 DirControl ( -1 0 1 1 ) 
 EmergencyStopToggle ( 0 1 0 ) 
 Headlights ( 0 0.25 1 0 ) 
 Horn ( 0 1 0 ) 
 PantographToggle1 ( 0 1 0 ) 
 PantographToggle2 ( 0 1 0 ) 
 Sanding ( 0 1 0 ) 
 Vigilance ( 0 1 0 ) 
 Wipers ( 0 1 0 ) 
 ) 
 
 Description ( 
 "Lokomotiva GySEV 1047 503-6/typ SIEMENS ES64 U2/,verze pro provoz na siti GySEV a MAVTR /HU/\n\n"+ 
 "Lokomotivy spolecnosti 'GySEV' rady 470 jsou prezdivany jako 'Taurus' a zajistuji vozbu vlaku "+ 
 "v Madarsku a sousednich statech\n\n"+ 
 "Maximalni rychlost lokomotivy : 230 km/h\n\n"+ 
 "Maximalni vykon lokomotivy : 6,4 MW\n\n"+ 
 "Vyska zdvihu sberacu tohoto modelu : 6,0 m\n\n"+ 
 "Lokomotiva je schopna jizdy na napajecich systemech : AC-25kV/50Hz, AC-15kV/16,7Hz.\n\n"+ 
 "Delka lokomotivy : 19 280 mm\n\n"+ 
 "Vaha lokomotivy : 86 t\n\n" 
 ) 
) 

