SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 193-820-8
	Type ( Engine ) 
	WagonShape ( 193-820-8.s ) 
	Freightanim ( 193-820-8_MS.s 1 1 ) 

	Size ( 3.012m 3.86m 18.98m ) 
	CentreOfGravity ( 0m 2.25m 0m ) 
	Mass ( 87t ) 
	WheelRadius ( 0.625m ) 
	InertiaTensor ( Box ( 3.012m 3.86m 18.98m ) ) 
 
	Coupling (
		Type ( Chain )
	Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 18cm 60cm )
		)
	CouplingHasRigidConnection ( 1 )
	Velocity ( 0.01m/s )
	)
 
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
 
	Adheasion ( 0.60 0.78 1.8 0 ) 
	DerailRailHeight ( 10cm ) 
	DerailRailForce ( 2.5*88t ) 
	DerailBufferForce ( 350kN ) 
	NumWheels ( 8 ) 
 
 	Friction ( 800N/m/s  0.05  1mph  6.2N/m/s  1.1  4.1N/rad/s  1  0.1rad/s  0.1N/rad/s  1 ) 

	AntiSlip ( 1 )

	BrakeEquipmentType ( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" ) 
	BrakeSystemType ( "Air_single_pipe" ) 

	MaxBrakeForce ( 105kN ) 
	MaxHandbrakeForce ( 25kN ) 
#	NumberOfHandbrakeLeverSteps ( ) 

	EmergencyBrakeResMaxPressure( 3.8bar )
#	TrainPipeLeakRate()
#	AuxilaryLeakRate()
	TripleValveRatio( 2.92 )
	MaxReleaseRate( 6 )
	MaxApplicationRate( 8 )
	MaxAuxilaryChargingRate( 40 )

	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 40 )

	BrakeCylinderPressureForMaxBrakeBrakeForce( 3.8bar ) 
	BrakeDistributorFullServicePressure( 3.4bar )
	BrakeDistributorMaxAuxilaryResPressure( 5bar )
	BrakeDistributorEmergencyResPressure( 3.8bar )
	BrakeDistributorReleaseRate( 11 )
	BrakeDistributorApplicationRate( 18 )
	BrakeDistributorTrainPipeControlRatio( 2.375 )
	BrakeDistributorNormalFullReleasePressure( 5bar )
 
 Lights ( 27
	comment( MEGVILAGITOTT TERULETEK )
		Light	(
			comment( MEGVILAGITOTT TERULET TOMPITOTT )
			Type ( 1 )
			Conditions (
			Headlight ( 2 )
			Unit ( 2 )
			Control ( 2 )
                        )
			Cycle	( 0 )
			FadeIn	( 0.2 )
			FadeOut	( 0.2 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 0.0 3.615 8.32 )
					Transition ( 0 )
					Radius ( 27.0 )
					Angle ( 38.0 )
					)
				)
			)
		Light	(
			comment( MEGVILAGITOTT TERULET REFLEKTOR )
			Type ( 1 )
			Conditions (
			Headlight ( 3 )
			Unit ( 2 )
			)
			Cycle	( 0 )
			FadeIn	( 0.8 )
			FadeOut	( 0.8 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffe8c0 )
					Position ( 0.0 3.615 8.32 )
					Transition ( 0 )
					Radius ( 61.0 )
					Angle ( 14.0 )
					)
				)
			)
	comment( ELSO FENYEK )
		Light	(
			comment( HOMLOK TOMPITOTT )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 0 3.615 8.32 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( 0 -20 0 )
					)
				)
			)
		Light	(
			comment( HOMLOK TOMPITOTT REV )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 0 3.615 -8.32 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( 0 -20 0 )
					)
				)
			)
		Light	(
			comment( HOMLOK REFLEKTOR )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 0 3.615 8.42 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
					Elevation ( 0 -36 0 )
					)
				)
			)
		Light	(
			comment( HOMLOK REFLEKTOR REV )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 0 3.615 -8.32 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.6 )
					Elevation ( 0 -36 0 )
					)
				)
			)
		Light	(
			comment( BAL ELSO TOMPITOTT )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( -1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 20.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( BAL ELSO TOMPITOTT REV)
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 20.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( JOBB ELSO TOMPITOTT)
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( JOBB ELSO TOMPITOTT REV)
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( -1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( BAL ELSO REFLEKTOR )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffe8c0 )
					Position ( -1.14 1.87 8.84 )
					Azimuth ( 0.0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( 20.0 10.0 0.0 )
					)
				)
			)
		Light	(
			comment( BAL ELSO REFLEKTOR REV )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffe8c0 )
					Position ( 1.14 1.87 -8.84 )
					Azimuth ( -180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( 20.0 10.0 0.0 )
					)
				)
			)
		Light	(
			comment( JOBB ELSO REFLEKTOR )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffe8c0 )
					Position ( 1.14 1.87 8.84 )
					Azimuth ( 0.0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( -20.0 10.0 0.0 )
					)
				)
			)
		Light	(
			comment( JOBB ELSO REFLEKTOR REV)
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffd080 )
					Position ( -1.14 1.87 -8.84 )
					Azimuth ( -180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( -20.0 10.0 0.0 )
					)
				)
			)
	comment( ZARFENYEK )
		Light	(
			comment( BAL HATSO ZARFENY )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)	
			)
		Light	(
			comment( BAL HATSO ZARFENY REV )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)	
			)
		Light	(
			comment( JOBB HATSO ZARFENY )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( JOBB HATSO ZARFENY REV )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( BAL HATSO ZARFENY )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)	
			)
		Light	(
			comment( BAL HATSO ZARFENY REV )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)	
			)
		Light	(
			comment( JOBB HATSO ZARFENY )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( JOBB HATSO ZARFENY REV )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
	comment( AI FENYEK )
		Light	(
			comment( HOMLOK TOMPITOTT AI )
			Type( 0 )
			Conditions (
				Control ( 1 )
				Unit ( 2 )
				Service ( 2 ) 
                       	TimeOfDay ( 0 ) 
				)

			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 0 3.615 8.32 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( 0 -20 0 )
					)
				)
			)
		Light	(
			comment( BAL ELSO TOMPITOTT AI )
			Type( 0 )
			Conditions (
				Control ( 1 )
				Unit ( 2 )
				Service ( 2 ) 
                       	TimeOfDay ( 0 ) 
				)

			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( -1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( JOBB ELSO TOMPITOTT AI )
			Type( 0 )
			Conditions (
				Control ( 1 )
				Unit ( 2 )
				Service ( 2 ) 
                       	TimeOfDay ( 0 ) 
				)

			FadeIn	( 0.1 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( fffff2dd )
					Position ( 1.15 1.67 8.74 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)	
		Light	(
			comment( BAL ZARFENY AI )
			Type( 0 )
			Conditions (
				Control ( 1 )
				Unit ( 3 )
				Service ( 2 ) 
                       	TimeOfDay ( 0 ) 
				)

			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)	
		Light	(
			comment( JOBB ZARFENY AI )
			Type( 0 )
			Conditions (
				Control ( 1 )
				Unit ( 3 )
				Service ( 2 ) 
                       	TimeOfDay ( 0 ) 
				)

			FadeIn	( 0.1 )
			FadeOut	( 0.1 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 1.15 1.67 -8.74 )
					Azimuth ( -180.0 -180.0 -180.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)

	)
 Sound ( "4700_eng.sms" ) 
 ) 

 
Engine ( 193-820-8
	Wagon ( 193-820-8 ) 
	Name ( "193-820-8" ) 
	Type ( Electric ) 

	MaxPower ( 6400kW )
	MaxForce ( 350kN )
	MaxContinuousForce ( 270kN )
	MaxCurrent ( 1200A ) 
	MaxVelocity ( 200km/h )
	WheelRadius ( 0.625m )
	Sanding ( 200km/h )
	
	ORTSDriveWheelWeight ( 11t )
	NumWheels ( 8 )

 	CabView ( "193.cvf" )
	HeadOut ( 1.5 3.08 6.6 ) 

    	Sound (	"4700_cab.sms" )
 
	AirBrakesAirCompressorPowerRating ( 1.8 ) 
	AirBrakesAirCompressorWattage ( 16000 ) 
	AirBrakesMainResVolume ( 1350l ) 
	AirBrakesMainMaxAirPressure ( 10bar ) 
	AirBrakesCompressorRestartPressure ( 8bar ) 
	AirBrakesMainMinResAirPressure ( 5.5bar ) 
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 1.5 ) 
	AirBrakesHasLowPressureTest ( 1 ) 
	AirBrakesIsCompressorElectricOrMechanical ( 0 ) 
 
	BrakesEngineControllers ( "Independent, Dynamic, Train" ) 
	BrakesEngineBrakeType ( "Air_twin_pipe"  )
	BrakesTrainBrakeType ( "Air_twin_pipe" )
 
	DoesBrakeCutPower ( 0 ) 
 
	EngineBrakesControllerDirectControlExponent ( 1 ) 
	EngineBrakesControllerHasProportionalBrake ( 0 ) 
	EngineBrakesControllerMaxReleaseRate ( 12 ) 
	EngineBrakesControllerMaxApplicationRate ( 10 ) 
	EngineBrakesControllerEmergencyApplicationRate ( 14 ) 
	EngineBrakesControllerMinSystemPressure ( 0 ) 
	EngineBrakesControllerMaxSystemPressure ( 3.8bar ) 
	EngineBrakesControllerFullServicePressureDrop ( 0.0bar ) 
	EngineBrakesProportionalBrakeLag ( 0.8 ) 
 
	TrainBrakesControllerMaxQuickReleaseRate ( 4.5 ) 
	TrainBrakesControllerMaxReleaseRate ( 4.0 ) 
	TrainBrakesControllerMaxApplicationRate ( 3.0 ) 
	TrainBrakesControllerEmergencyApplicationRate ( 18 ) 
	TrainBrakesControllerMinPressureReduction ( 4.5 ) 
	TrainBrakesControllerFullServicePressureDrop ( 1.6bar ) 
	TrainBrakesControllerMinSystemPressure ( 0 ) 
	TrainBrakesControllerMaxSystemPressure ( 73 ) 
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
	TrainPipeLeakRate ( 0.033 ) 
 
	DynamicBrakesResistorCurrentLimit ( 1200 ) 
	DynamicBrakesDelayTimeBeforeEngaging ( 0 ) 
	DynamicBrakesNumberOfControllerNotches ( 10 ) 
	DynamicBrakesMaxAirBrakePressure ( 55 ) 
	DynamicBrakeHasAutoBailOff ( 0 ) 
	DynamicBrakesMaximumForce ( 150kN ) 
	DynamicBrakesHigherSpeedCurveExponent ( 2 ) 
	DynamicBrakesLowerSpeedCurveExponent ( 2 ) 
	DynamicBrakesMaximumSpeedForFadeOut ( 430 ) 
	DynamicBrakesMaximumEffectiveSpeed ( 97 ) 
	DynamicBrakesFadingSpeed ( 9 ) 
	DynamicBrakesMinUsableSpeed ( 2 ) 
	DynamicBrakesCutInSpeed ( 2 ) 
	DynamicBrakesCutOutSpeed ( 2 ) 
	DynamicBrakesEffectAtMaximumFadeOut ( 1 ) 
 
OverspeedMonitor ( 
	MonitoringDeviceMonitorTimeLimit ( 0 ) 
	MonitoringDeviceAlarmTimeLimit ( 5 ) 
	MonitoringDevicePenaltyTimeLimit ( 0 ) 
	MonitoringDeviceCriticalLevel ( 165 ) 
	MonitoringDeviceResetLevel ( 0 ) 
	MonitoringDeviceTriggerOnHighCurrent ( 1250 ) 
	MonitoringDeviceAppliesFullBrake ( 0 ) 
	MonitoringDeviceAppliesEmergencyBrake ( 0 ) 
	MonitoringDeviceAppliesCutsPower ( 1 ) 
	MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
	MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 ) 
	MonitoringDeviceDoesSuppressionReset ( 0 ) 
	MonitoringDeviceResetOnZeroSpeed ( 1 ) 
	MonitoringDeviceResetOnDirectionNeutral ( 1 ) 
) 
VigilanceMonitor ( 
	MonitoringDeviceMonitorTimeLimit ( 31.2 )
	MonitoringDeviceAlarmTimeLimit ( 23 )
	MonitoringDevicePenaltyTimeLimit ( 0 ) 
	MonitoringDeviceCriticalLevel ( 0 ) 
	MonitoringDeviceResetLevel ( 0 ) 
	MonitoringDeviceAppliesFullBrake ( 1 ) 
	MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
	MonitoringDeviceAppliesCutsPower ( 0 ) 
	MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
	MonitoringDeviceResetOnZeroSpeed ( 1 ) 
	MonitoringDeviceResetOnResetButton ( 1 ) 
) 
EmergencyStopMonitor ( 
	MonitoringDeviceMonitorTimeLimit ( 0 ) 
	MonitoringDeviceAlarmTimeLimit ( 0 ) 
	MonitoringDevicePenaltyTimeLimit ( 0 ) 
	MonitoringDeviceCriticalLevel ( 0 ) 
	MonitoringDeviceResetLevel ( 0 ) 
	MonitoringDeviceAppliesFullBrake ( 1 ) 
	MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
	MonitoringDeviceAppliesCutsPower ( 1 ) 
	MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
	MonitoringDeviceResetOnZeroSpeed ( 1 ) 
	MonitoringDeviceResetOnResetButton ( 1 ) 
) 
		 
EngineControllers ( 
 
	Throttle ( 0 1 0.2 0 
		NumNotches ( 1 
			Notch ( 0 1 Dummy ) 
		)
	)
 	Brake_Dynamic ( 0 1 0.2 0 
		NumNotches ( 0 )
	)
	Brake_Engine ( 0 1 0.1 0 
		NumNotches ( 1
			Notch ( 0       1 Dummy )                    
		)
	)
	Brake_Train ( 0 1 0.1 0.2 
		NumNotches ( 6 
			Notch ( 0.0 0 TrainBrakesControllerFullQuickReleaseStart ) 
			Notch ( 0.1 0 TrainBrakesControllerReleaseStart ) 
			Notch ( 0.2 0 TrainBrakesControllerNeutralhandleOffStart ) 
			Notch ( 0.3 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart ) 
			Notch ( 0.9 0 TrainBrakesControllerSuppressionStart ) 
			Notch ( 1.0 0 TrainBrakesControllerEmergencyStart ) 
		)
	) 
	Combined_Control( 0 1 0.125 0 throttle dynamic )
	AWS ( 0 1 0 )
	BailOffButton( 0 1 0 )
	BellToggle( 0 1 0 )
	DirControl ( -1 0 1 1 )
	EmergencyStopResetToggle( 0 1 0 )
	EmergencyStopToggle( 0 1 0 )
	Headlights ( 0 0.25 1 0 )
	Horn ( 0 1 0 )
	Sanding ( 0 1 0 )
	Vigilance ( 0 1 0 )
	Wipers ( 0 1 0 )
   )
 
 Description ( 
	"Gyártó: Siemens AG\n\n"+
	"Gyártási típus: X4e\n\n"+
	"Gyártási év: 2010-\n\n"+
	"Áramnem: 15 kV / 16,7 Hz és 25 kV / 50 Hz\n\n"+
	"Állandó teljesítmény: 1.640 kW x4 (6,4MW)\n\n"+
	"Jármű maximumsebesség: 200 km/h\n\n"+
	"Új kerékátmérő 1.150 mm\n\n"+
	"Legnagyobb magasság (Leengedett áramszedő mellett): 3.860 mm\n\n"+
	"Legnagyobb szélesség (mozdonyszekrény): 3.012 mm\n\n"+
	"Legnagyobb hosszúság (ütközök közötti): 18.980 mm\n\n"+
	"Szolgálati tömeg új kerékpárokkal 2/3 homokkiszereléssel: 87t ± 1%\n\n"+
	"Tengelyelrendezés Bo’Bo’"
 ) 
) 
