SIMISA@@@@@@@@@@JINX0D0t______
 
Wagon ( obb_Afmpz_713_de
 Type ( Engine ) 
 WagonShape ( obb_Afmpz_713_de.s ) 
 Freightanim ( obb_Afmpz_713_fa.s 1 1 )
 
 
Comment ( Pozice svetel : Jiri Tovacovsky ) 
Comment ( Verze ladeni ENG: bob57_cz , 10.9.2011 ) 
 
 Size ( 2.83m 4.06m 25.65m )
 CentreOfGravity ( 0m 2.25m 0m ) 
 Mass ( 53t ) 
 WheelRadius ( 0.625m ) 
 InertiaTensor ( Box ( 2.83m 4.06m 25.65m ) ) 
 
 Coupling ( 
  Type ( Chain ) 
   Spring ( 
    Stiffness ( 7.5e6N/m 1e7N/m ) 
    Damping ( 1e6N/m/s 2e6N/m/s ) 
    Break ( 1.1e8N 5e8N ) 
    r0 ( 80cm 150cm ) 
    ) 
 CouplingHasRigidConnection ( 0 ) 
 Velocity ( 0.01m/s ) 
 ) 
 
 Buffers ( 
  Spring ( 
   Stiffness ( 1e6N/m 5e6N/m ) 
   Damping ( 1e6N/m/s 1e6N/m/s ) 
   r0 ( 6cm 30cm ) 
   ) 
   Centre ( 0.5 ) 
   Radius ( 1 ) 
   Angle ( 0.5deg ) 
 ) 
 
 Adheasion ( 0.60 0.78 1.8 0 ) 
 DerailRailHeight ( 10cm ) 
 DerailRailForce ( 2.5*53t ) 
 DerailBufferForce ( 350kN ) 
 NumWheels ( 4 ) 
 
 Friction ( 800N/m/s  0.05  1mph  6.2N/m/s  1.2  4.1N/rad/s  1  0.1rad/s  0.1N/rad/s  1 ) 
 
 BrakeEquipmentType ( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake, Emergency_brake_reservoir" ) 
 BrakeSystemType ( "Air_single_pipe" ) 
 MaxBrakeForce ( 105kN ) 
 MaxHandbrakeForce ( 25kN ) 
 NumberOfHandbrakeLeverSteps ( 100 ) 
 BrakeCylinderPressureForMaxBrakeBrakeForce ( 56 ) 
 EmergencyBrakeResMaxPressure ( 72 ) 
 TripleValveRatio ( 2.53 ) 
 MaxReleaseRate ( 2 ) 
 MaxApplicationRate ( 2 ) 
 MaxAuxilaryChargingRate ( 2 ) 
 EmergencyResChargingRate ( 2 ) 
 EmergencyResVolumeMultiplier ( 2 ) 
 EmergencyResCapacity ( 0.3 ) 
 
	Lights ( 29 
 
Comment ( svetelne kuzely ) 

 Light ( comment ( 1 svetelny kuzel obrysove ) 
  Type ( 1 ) 
  Conditions ( 
  Headlight ( 1 ) 
  Unit ( 2 ) 
  Control ( 2 ) 
  TimeOfDay ( 2 ) 
  ) 
  FadeIn ( 0.1 ) 
  FadeOut ( 0.1 ) 
  Cycle ( 0 ) 
  States ( 1 
  State ( 
   Duration ( 0 ) 
   LightColour ( 16161616  ) 
   Position ( 0.0 1.7 -1.4 ) 
   Transition ( 0 )
   Angle ( 10 ) 
   Radius ( 20 ) 
 ) ) ) 
 
 Light ( Comment ( 2 Svetelny kuzel tlumeny ) 
  Type ( 1 ) 
  Conditions ( 
  Headlight ( 2 ) 
  Unit ( 2 ) 
  Control ( 2 ) 
  TimeOfDay ( 2 ) 
  ) 
  FadeIn ( 0.1 ) 
  FadeOut ( 0.1 ) 
  Cycle ( 0 ) 
  States ( 1 
  State ( 
   Duration ( 0 ) 
   LightColour ( 8b80734b ) 
   Position ( 0 3.5 8.8 ) 
   Transition ( 0 )
   Angle ( 10 ) 
   Radius ( 250 ) 
 ) ) ) 
 
 Light ( Comment ( 3 Svetelny kuzel dalkovy ) 
  Type ( 1 ) 
  Conditions ( 
  Headlight ( 3 ) 
  Unit ( 2 ) 
  Control ( 2 ) 
  ) 
  FadeIn ( 0.1 ) 
  FadeOut ( 0.1 ) 
  Cycle ( 0 ) 
  States ( 1 
  State ( 
   Duration ( 0 ) 
   LightColour ( fcf0e68c ) 
   Position ( 0 3.5 8.8 ) 
   Transition ( 0 )
   Angle ( 10 ) 
   Radius ( 250 ) 
 ) ) ) 
 
Comment ( Definice svetel pro predni stanoviste v cele vlaku )

		Light (
			Comment ( Predni reflektor dalkovy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 3.587 12.115 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -40 -40 -40 )
				)
			)
		)

		Light (
			Comment ( Predni reflektor pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 3.587 12.115 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -40 -40 -40 )
				)
			)
		)

		Light (
			Comment ( Predni reflektor pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 3.587 12.115 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -40 -40 -40 )
				)
			)
		)

		Light (
			Comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.667 12.715 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 1 )
				Unit ( 0 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.667 12.715 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.897 12.715 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.897 12.715 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.897 12.715 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 2 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.897 12.715 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

				
Comment ( Definice svetel pro predni stanoviste na postrku )

		Light (
			Comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( 1.14 1.667 -12.715 )
					Azimuth ( -180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( -1.14 1.667 -12.715 )
					Azimuth ( -180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

Comment ( Definice svetel pro zadni stanoviste v cele vlaku )
		
		Light (
			Comment ( Reflektor dalkovy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
				Service( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 3.587 -12.115 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -40 -40 -40 )
				)
			)
		)

		Light (
			Comment ( Reflektor pozicni )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 3.587 -12.115 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -40 -40 -40 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.897 -12.715 )
					Azimuth ( 180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 2 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.897 -12.715 )
					Azimuth ( 180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni prave dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.897 -12.715 )
					Azimuth ( 180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( Predni leve dalkove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 3 )
				Unit ( 5 )
				Service ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.897 -12.715 )
					Azimuth ( 180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		
Comment ( Definice svetel pro zadni stanoviste na postrku )
		
		Light (
			Comment ( Zadni prave koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( 1.14 1.667 12.715 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light ( 
			Comment ( Zadni leve koncove )
			Type ( 0 )
			Conditions ( 
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( ffff0000 )
					Position ( -1.14 1.667 12.715 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

Comment ( Definice svetel pro loko ovladanou PC v normalnim smeru )

		Light (
			Comment ( PC predni prave v soupravy normalni smer )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.667 12.715 )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
		Light (
			Comment ( PC predni leve v cele soupravy normalni smer )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.667 12.715 )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)

		Light (
			Comment ( PC koncove prave na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.667 -12.715 )
					Azimuth ( -180.0 150.0 165.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 20 )
				)
			)
		)
		
		Light (
			comment ( PC pozicni leve na konci soupravy )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.667 -12.715  )
					Azimuth ( -180.0 -165.0 -150.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
Comment ( Definice svetel pro Loose consist )

		Light (
			Comment ( Reflektor pozicni - Loose consist )
			Type ( 0 )
			Conditions ( 
				Headlight ( 0 )
				Service ( 0 )
				Control ( 1 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle ( 0 )
			States ( 1
				State ( 
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 0 3.587 12.115 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -40 -40 -40 )
				)
			)
		)

		Light	(
			Comment( Predni prave pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( 1.14 1.667 12.715  )
					Azimuth ( 0 30.0 15.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
		
		Light	(
			Comment( Predni leve pozicni - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.1 )
			FadeOut ( 0.1 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0 )
					LightColour ( fcf0e68c )
					Position ( -1.14 1.667 12.715  )
					Azimuth ( 0 -15.0 -30.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					Elevation ( -20 -20 -20 )
				)
			)
		)
	) 

 Sound ( "..//..//common.snd//sndElok//obbafmpzeng.sms" ) 
 ) 
 
Engine ( obb_Afmpz_713_de 
 Wagon ( obb_Afmpz_713_de ) 
 Type ( Electric ) 
 Name ( "OBB_RJ_Afmpz_713-6_DE" )  
 MaxPower ( 64W ) 
 MaxForce ( 300N ) 
 MaxContinuousForce ( 300N ) 
 MaxCurrent ( 12A ) 
 MaxVelocity ( 253km/h ) 
 DieselEngineSpeedOfMaxTractiveEffort ( 255km/h ) 
 WheelRadius ( 0.625m ) 
 Sanding ( 200km/h ) 
 NumWheels ( 4 ) 
 Sound ( "..//..//common.snd//sndElok//obbafmpz_SIFA_cab.sms" ) 
 CabView ( "..//..//common.cab//cabobbafmpz//afmpz_de.cvf" ) 
 HeadOut ( 1.7 3 11.2 ) 
 
 AirBrakesAirCompressorPowerRating ( 1.2 ) 
 AirBrakesAirCompressorWattage ( 16000 ) 
 AirBrakesMainResVolume ( 40 ) 
 AirBrakesMainMaxAirPressure ( 145 ) 
 AirBrakesCompressorRestartPressure ( 116 ) 
 AirBrakesMainMinResAirPressure ( 73 ) 
 AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 4 ) 
 AirBrakesHasLowPressureTest ( 1 ) 
 AirBrakesIsCompressorElectricOrMechanical ( 0 ) 
 
 BrakesEngineControllers ( "Dynamic, Independent, Train" ) 
 BrakesEngineBrakeType ( "Air_single_pipe" ) 
 BrakesTrainBrakeType ( "Air_single_pipe" ) 
 
 DoesBrakeCutPower ( 1 ) 
 
 EngineBrakesControllerHasProportionalBrake ( 1 ) 
 EngineBrakesControllerMaxReleaseRate ( 5 ) 
 EngineBrakesControllerMaxApplicationRate ( 5 ) 
 EngineBrakesControllerEmergencyApplicationRate ( 10 ) 
 EngineBrakesControllerMinSystemPressure ( 0 ) 
 EngineBrakesControllerMaxSystemPressure ( 73 ) 
 EngineBrakesControllerFullServicePressureDrop ( 73 ) 
 EngineBrakesControllerDirectControlExponent ( 1 ) 
 EngineBrakesProportionalBrakeLag ( 0.8 ) 
 
 TrainBrakesControllerMaxQuickReleaseRate ( 1.5 ) 
 TrainBrakesControllerMaxReleaseRate ( 0.5 ) 
 TrainBrakesControllerMaxApplicationRate ( 1 ) 
 TrainBrakesControllerEmergencyApplicationRate ( 10 ) 
 TrainBrakesControllerMinPressureReduction ( 3 ) 
 TrainBrakesControllerFullServicePressureDrop ( 28 ) 
 TrainBrakesControllerMinSystemPressure ( 0 ) 
 TrainBrakesControllerMaxSystemPressure ( 73 ) 
 TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 ) 
 TrainPipeLeakRate ( 0.033 ) 
 
 DynamicBrakesResistorCurrentLimit ( 12 ) 
 DynamicBrakesDelayTimeBeforeEngaging ( 0 ) 
 DynamicBrakesNumberOfControllerNotches ( 10 ) 
 DynamicBrakesMaxAirBrakePressure ( 55 ) 
 DynamicBrakeHasAutoBailOff ( 0 ) 
 DynamicBrakesMaximumForce ( 150N ) 
 DynamicBrakesHigherSpeedCurveExponent ( 2 ) 
 DynamicBrakesLowerSpeedCurveExponent ( 2 ) 
 DynamicBrakesMaximumSpeedForFadeOut ( 430 ) 
 DynamicBrakesMaximumEffectiveSpeed ( 97 ) 
 DynamicBrakesFadingSpeed ( 9 ) 
 DynamicBrakesMinUsableSpeed ( 2 ) 
 DynamicBrakesCutInSpeed ( 2 ) 
 DynamicBrakesCutOutSpeed ( 2 ) 
 DynamicBrakesEffectAtMaximumFadeOut ( 1 )  
 
 OverspeedMonitor ( 
  MonitoringDeviceMonitorTimeLimit ( 0 ) 
  MonitoringDeviceAlarmTimeLimit ( 5 ) 
  MonitoringDevicePenaltyTimeLimit ( 0 ) 
  MonitoringDeviceCriticalLevel ( 0 ) 
  MonitoringDeviceResetLevel ( 0 ) 
  MonitoringDeviceTriggerOnHighCurrent ( 1250 ) 
  MonitoringDeviceAppliesFullBrake ( 0 ) 
  MonitoringDeviceAppliesEmergencyBrake ( 0 ) 
  MonitoringDeviceAppliesCutsPower ( 1 ) 
  MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
  MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 ) 
  MonitoringDeviceDoesSuppressionReset ( 0 ) 
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnDirectionNeutral ( 1 ) 
 ) 
 VigilanceMonitor ( 
  MonitoringDeviceMonitorTimeLimit ( 27 ) 
  MonitoringDeviceAlarmTimeLimit ( 17 ) 
  MonitoringDevicePenaltyTimeLimit ( 0 ) 
  MonitoringDeviceCriticalLevel ( 0 ) 
  MonitoringDeviceResetLevel ( 0 ) 
  MonitoringDeviceAppliesFullBrake ( 0 ) 
  MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
  MonitoringDeviceAppliesCutsPower ( 1 ) 
  MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 1 ) 
 ) 
EmergencyStopMonitor ( 
  MonitoringDeviceMonitorTimeLimit ( 0 ) 
  MonitoringDeviceAlarmTimeLimit ( 0 ) 
  MonitoringDevicePenaltyTimeLimit ( 0 ) 
  MonitoringDeviceCriticalLevel ( 0 ) 
  MonitoringDeviceResetLevel ( 0 ) 
  MonitoringDeviceAppliesFullBrake ( 1 ) 
  MonitoringDeviceAppliesEmergencyBrake ( 1 ) 
  MonitoringDeviceAppliesCutsPower ( 1 ) 
  MonitoringDeviceAppliesShutsDownEngine ( 0 ) 
  MonitoringDeviceResetOnZeroSpeed ( 1 ) 
  MonitoringDeviceResetOnResetButton ( 1 ) 
  ) 
		 
EngineControllers ( 
 
 Throttle ( 0 1 0.02 0 
 NumNotches ( 1 
 Notch ( 0 1 Dummy ) 
 ) ) 
 
 Brake_Dynamic ( 0 1 0.05 0 
 NumNotches ( 10 
 Notch ( 0.00 0 Dummy ) 
 Notch ( 0.15 0 Dummy ) 
 Notch ( 0.20 0 Dummy ) 
 Notch ( 0.30 0 Dummy ) 
 Notch ( 0.45 0 Dummy ) 
 Notch ( 0.55 0 Dummy ) 
 Notch ( 0.65 0 Dummy ) 
 Notch ( 0.75 0 Dummy ) 
 Notch ( 0.85 0 Dummy ) 
 Notch ( 1.00 0 Dummy ) 
 ) )
 
 Brake_Engine ( 0 1 0.1 0 
 NumNotches ( 1 
 Notch ( 0 1 Dummy ) 
 ) ) 
 
 Brake_Train ( 0 1 0.1 0.2 
 NumNotches ( 6 
 Notch ( 0.0 0 TrainBrakesControllerFullQuickReleaseStart ) 
 Notch ( 0.1 0 TrainBrakesControllerReleaseStart ) 
 Notch ( 0.2 0 TrainBrakesControllerNeutralhandleOffStart ) 
 Notch ( 0.3 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart ) 
 Notch ( 0.9 0 TrainBrakesControllerSuppressionStart ) 
 Notch ( 1.0 0 TrainBrakesControllerEmergencyStart ) 
 ) ) 
 
 AWS ( 0 1 0 ) 
 BailOffButton ( 0 1 0 ) 
 BellToggle ( 0 1 0 ) 
 DirControl ( -1 0 1 1 ) 
 EmergencyStopToggle ( 0 1 0 ) 
 Headlights ( 0 0.25 1 0 ) 
 Horn ( 0 1 0 ) 
 PantographToggle1 ( 0 1 0 ) 
 PantographToggle2 ( 0 1 0 ) 
 Sanding ( 0 1 0 ) 
 Vigilance ( 0 1 0 ) 
 Wipers ( 0 1 0 ) 
 ) 
 
 Description ( 
 "Ridici vuz OBB "RJ" Afmpz 713-6 ,verze pro provoz na siti DB /DE/.\n\n"+ 
 "Ridici vozy OBB Afmpz jsou razeny v soupravach "RailJet" Rakouskych spolkovych drah /OBB/.\n\n"+ 
 "Maximalni rychlost ridiciho vozu : 230 km/h\n\n"+ 
 "Delka ridiciho vozu : 26 850 mm\n\n"+ 
 "Vaha ridiciho vozu : 50.9 t\n\n" 
 ) 
) 
