SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 193-206
	Type ( Engine )
	WagonShape ( 193-206.s )
 	FreightAnim ( 193-206_anim.s 1 1 )
	Size  ( 3m 4m 19.42m )
	CentreOfGravity ( 0m 1.668m 0m )
	Mass ( 87t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box ( 3m 4m 19m ) )
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1.1e6N/m 4.8e6N/m )
			Damping ( 1.2e6N/m/s 3.4e6N/m/s )
			Break ( 3.4e7N 3.4e7N )
			r0 ( 20cm 30cm )
		)
		CouplingHasRigidConnection ()
		Velocity ( 0.15m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 4.8e6N/m 1.1e6N/m )
			Damping ( 3.4e6N/m/s 1.2e6N/m/s )
			Break ( 3.4e7N 3.4e7N )
			r0 ( 30cm 20cm )
		)
		CouplingHasRigidConnection ()
		Velocity ( -0.15m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e7N/m 0 )
			Damping ( 1e6N/m/s 0 )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5m )
		Radius ( 1m )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.25 0.44 2 0 )
	DerailRailHeight ( 5cm )
	DerailRailForce ( 435kN )
	DerailBufferForce ( 250kN )
	NumWheels (	1 )
	Friction (
		comment( values by Joseph Realmuto FCalc 2.0 )
		comment( entered values are: L,F,R,4,87,11,0.6;Y,87 )
		1070.5N/m/s		-0.10		1.2mph		8.893N/m/s		1.822
		5.1N/rad/s		1		-1rad/s		0		1
	)
	AntiSlip ()
 	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Emergency_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 180kN )

	EmergencyBrakeResMaxPressure( 72 )
	TripleValveRatio( 3 )
	MaxReleaseRate( 4 )
	MaxApplicationRate( 5 )
	MaxAuxilaryChargingRate( 5 )
	EmergencyResCapacity( 4 )
	EmergencyResChargingRate( 5 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 54 )
	BrakeAirPressureGainInResForOnePoundFromPipe( 0.5 )

      Lights	(	12
		Light	(
			comment( TOP Sphere of light )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffff99 )
					Position ( 0.0 3.602 9.015 )
					Transition ( 0 )
					Radius ( 120.0 )
					Angle ( 15.0 )
					)
				)
			)
		Light	(
			comment( FRONT Head top light )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffff99 )
					Position ( 0.0 3.671 8.9 )
					Azimuth ( 0 -15 0 )
					Elevation ( -50 -50 -50 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( FRONT left light )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffff99 )
					Position ( -1.2 1.65 9.35 )
					Transition ( 0 )
					Radius ( 0.3 )
					Azimuth ( 0 -40 10 )
					Elevation ( 0 -25 25 )
					)
				)
			)
		Light	(
			comment( FRONT right light )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffff99 )
					Position ( 1.2 1.65 9.35 )
					Transition ( 0 )
					Radius ( 0.3 )
					Azimuth ( 0 -10 40 )
					Elevation ( 0 -25 25 )
					)
				)
			)
		Light	(
			comment( FRONT left red light)
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.2 1.9 9.39 )
					Azimuth ( 0 -40 10 )
					Elevation ( 0 -25 25 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( FRONT right red light)
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.2 1.9 9.39 )
					Azimuth ( 0 -10 40 )
					Elevation ( 0 -25 25 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( REAR Head top light )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffff99 )
					Position ( 0.0 3.671 -8.9 )
					Azimuth ( -180 -170 -180 )
					Elevation ( -50 -50 -50 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( REAR left light )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 5 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffff99 )
					Position ( -1.2 1.65 -9.35 )
					Azimuth ( -180 -150 -180 )
					Elevation ( 0 -25 25 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment( REAR right light )
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 5 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffff99 )
					Position ( 1.2 1.65 -9.35 )
					Azimuth ( -180 150 180 )
					Elevation ( 0 -25 25 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		Light	(
			comment ( REAR left red light )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -1.2 1.9 -9.39 )
					Azimuth ( -180 -180 -140 )
					Elevation ( 0 -25 25 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
            Light	(
			comment ( REAR right red light  )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 1.2 1.9 -9.39 )
					Azimuth ( -180 140 180 )
					Elevation ( 0 -25 25 )
					Transition ( 0 )
					Radius ( 0.3 )
                              )
                        )
			)
		Light	(
			comment( Pantograph flash )
			Type		( 0 )
			Conditions	(
				Headlight ( 0 )
				Unit ( 3 )
				)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8
				State	(
					Duration ( 4.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 1.30 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 15.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 7.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( 11000000 )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.5 -5.3 )
					Azimuth ( 0.0 -180.0 180.0)
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				)
			)
		)
	Sound (	4700eng.sms )
)

Engine ( 193-206
    Wagon ( 193-206 )
    Type ( Electric )
    MaxPower ( 4684kW )
    MaxForce ( 300kN )
    MaxContinuousForce ( 300kN )
    MaxVelocity ( 160kmh )
    MaxCurrent ( 300A )
    WheelRadius ( 0.625m )
    Sanding ( 6mph )
    NumWheels ( 1 )

    CabView ( Vectron.cvf )
    HeadOut ( 1.7 3.0 7.75 )
	MaxTemperature ( 120 )
	MaxOilPressure ( 90 )

    AirBrakesAirCompressorPowerRating( 3.5 )
    AirBrakesMainMinResAirPressure( 0 )
    AirBrakesMainMaxAirPressure( 72 )
    AirBrakesMainResVolume( 28 )
    AirBrakesAirCompressorWattage( 10000 )
    AirBrakesCompressorRestartPressure( 67 )
    AirBrakesAirUsedPerPoundsOfBrakePipePressure( 1.5 )
    AirBrakesHasLowPressureTest ( 1 )
    AirBrakesIsCompressorElectricOrMechanical( 0 )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 7 )
 	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 72 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 5 )
	EngineBrakesControllerFullServicePressureDrop( 26 )
      EngineBrakesControllerMinPressureReduction( 1 )
	EngineBrakesControllerMaxReleaseRate( 7 )
	EngineBrakesControllerEmergencyApplicationRate( 40 )
	EngineBrakesControllerDirectControlExponent( 1 )

	TrainBrakesControllerMinPressureReduction( 1 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 40 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerFullServicePressureDrop( 26 )

    DynamicBrakesMinUsableSpeed( 5 )
    DynamicBrakesMaximumEffectiveSpeed( 25 )
    DynamicBrakesMaximumForce( 150kN )
    DynamicBrakesResistorCurrentLimit ( 326A )
    DynamicBrakesCutInSpeed( 1 )
    DynamicBrakesMaxAirBrakePressure ( 55 )
    DynamicBrakesFadingSpeed( 45 )
    DynamicBrakesDelayTimeBeforeEngaging ( 0 )
    DynamicBrakesMaximumSpeedForFadeOut ( 95 )
    DynamicBrakesEffectAtMaximumFadeOut( 1 )
    DynamicBrakesHigherSpeedCurveExponent( 1 )
    DynamicBrakesLowerSpeedCurveExponent( 1 )
    DynamicBrakesNumberOfControllerNotches( 11 )

	BrakesEngineBrakeType( "Air_single_pipe" )
	BrakesTrainBrakeType( "Air_single_pipe" )
        BrakesEngineControllers( "Independent, Train, Dynamic" )
    
	DoesBrakeCutPower( 1 )
      DoesHornTriggerBell( 0 )
	DieselEngineSpeedOfMaxTractiveEffort ( 13mph )
      BrakeCutsPowerAtBrakeCylinderPressure( 14 )
    
	EmergencyStopMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 0 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
	)

	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 45 )
		MonitoringDeviceAlarmTimeLimit( 37 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceResetOnZeroSpeed( 1 ) 
		MonitoringDeviceResetOnResetButton( 1 )
	)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 97 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 1 ) 
		MonitoringDeviceResetOnResetButton( 1 )
	)

        EngineControllers (
            Throttle ( 0 1 0.034 0 
                NumNotches ( 0 )
            )
            Brake_Engine ( 0 1 0.125 0 
                NumNotches ( 3
                   Notch ( 0        0 EngineBrakesControllerReleaseStart ) 
                   Notch ( 0.1     1 EngineBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                   Notch ( 0.95    0 EngineBrakesControllerFullServiceStart )
                )
            )
           Brake_Train ( 0 1 0.05 0.2 
                NumNotches ( 6
			    Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
			    Notch ( 0.1 0 TrainBrakesControllerReleaseStart )
 		   	    Notch ( 0.2 0 TrainBrakesControllerHoldLappedStart )
			    Notch ( 0.3 1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
			    Notch ( 0.9 0 TrainBrakesControllerContinuousServiceStart )
			    Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
                )
            )
 		Brake_Dynamic ( 0 1 0.01 0 
 		  NumNotches ( 11
                   Notch ( 0        0 Dummy )
                   Notch ( 0.1        0 Dummy )
                   Notch ( 0.2        0 Dummy )
                   Notch ( 0.3        0 Dummy )
                   Notch ( 0.4       0 Dummy )
                   Notch ( 0.5        0 Dummy )
                   Notch ( 0.6        0 Dummy )
                   Notch ( 0.7        0 Dummy )
                   Notch ( 0.8        0 Dummy )
                   Notch ( 0.9        0 Dummy )
                   Notch ( 1.0        0 Dummy )
 		  )
		)
        DirControl ( -1 0 1 1 )
        EmergencyStopResetToggle( 0 1 0 )
        EmergencyStopToggle( 0 1 0 )
        AWS ( 0 1 0 )
        Sanding ( 0 1 0 )
        Horn ( 0 1 0 )
        Vigilance ( 0 1 0 )
        PantographToggle1 ( 0 1 1 )
        PantographToggle2 ( 0 1 0 )
        PantographToggle_4 ( 0 1 1 )
        Headlights ( 0 0.25 1 0 )
        Wipers ( 0 1 0 )
        BellToggle( 0 1 0 )
        BailOffButton( 0 1 0 )
    )

     Sound ( 4700wag.sms )
   Name ( "Vectron, 193-206" )
    Description (
	"Locomotiva Eléctrica de Via Larga\n"+
	"CP serie 4700\n"+
	"Locomotiva de Carga.\n\n"+
	"Potecia: 4600 kW\n\n"+
	"V. Max: 140 Km/h (87 mph)\n\n"+
	"Ano de Construcao 2007-2009\n\n"+
	"Entrada ao Servico: 2008"
    )
    EngineOperatingProcedures (
    "To move forward\n"+
    "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
    "2.	Press the W key to move the Reverser to Forward.\n"+
    "3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
    "4.	Press the D key to move increase the throttle setting.\n\n"+  
    "To slow the train\n"+
    "1.	Press the A key to move the throttle to a lower setting.\n"+
    "2.	Use the brakes to further reduce speed if desired.\n\n"+   
    "To apply the train brakes\n"+
    "1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
    "To release the train brakes\n"+
    "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
    "To activate emergency braking\n"+
    "1.	Press the A key to reduce the throttle to Idle.\n"+
    "2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
    "To back up\n"+
    "1.	Bring your train to a full stop.\n"+
    "2.	Press the S key to move the Reverser to the Reverse position.\n"+
    "3.	Press the ; (SEMICOLON)  to release the brakes.\n"+
    "4.	Slowly advance the throttle lever (D key).\n\n"+
    "To load and unload passengers\n"+
    "1. Stop at a station.\n"+
    "2. Press the ENTER key.\n"+
    "3. Wait for the 'permission to depart' signal.\n"+
    "TIP: Use the Next Station driving aid (F10) to monitor loading and unloading."
    ) 
)