SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( H-Start_90_55_90-76_003-9
	Type ( Engine )
	WagonShape ( H-Start_90_55_90-76_003-9.s )
        Size  ( 3.101m 4.335m 26.0m )
	CentreOfGravity ( 0.0m 0.0m 0.0m )
	Mass ( 74t )
	WheelRadius ( 0.5m )
	InertiaTensor ( Box ( 3.101m 4.335m 26.361m ) )

comment ( Rear Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
	CouplingHasRigidConnection ( 0 )
	Velocity ( 0.01m/s )
	)
	
comment ( Front Coupler )

	Coupling (
		Type ( Chain )
		Spring (
		   Stiffness ( 7.5e6N/m 1e7N/m )
		   Damping ( 1e6N/m/s 2e6N/m/s )
		   Break ( 1.1e8N 5e8N )
		   r0 ( 3cm 13cm )
		)
        CouplingHasRigidConnection ( 0 )
        Velocity ( 0.01m/s )
	)

	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 6cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.2 0.4 1 0 ) comment ( MSTS default ertekek )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 400*2.5t )
	DerailBufferForce ( 2000kN )
	NumWheels ( 8 )
	Friction (
		150N/m/s		1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)
	AntiSlip ()

	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	
	MaxBrakeForce( 89kN ) comment ( V63 fektablazata alapjan: K: 20t, TT: 49t, T: 56t, Sz: 89t, N: 139t )
	MaxHandbrakeForce( 20kN )
#	NumberOfHandbrakeLeverSteps()

	EmergencyBrakeResMaxPressure( 55.1 ) comment ( Ilyen nincs valosagban a V43-ason, 3.8bar = 55.1psi )
#	TrainPipeLeakRate()
#	AuxilaryLeakRate()
	TripleValveRatio( 2.92 ) comment ( Dokumentacio szerint: 3.8bar[fekheng]/{5bar[fovez-toltott]-3.4[fovez-min]} [1/101],[4/284] )
	MaxReleaseRate( 11 ) comment  ( 5 s fekhenger uritesi ido 55psi/5s = 11psi/s csak mozdonyra /becsult/ )
	MaxApplicationRate( 18 ) comment ( 3 s fekhenger toltesi ido 55psi/3s = 18psi/s csak mozdonyra /becsult/ )
	MaxAuxilaryChargingRate( 40 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 40 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 55.1 ) comment ( 3.8bar = 55.1psi )

	BrakeDistributorFullServicePressure( 82 )
	BrakeDistributorMaxAuxilaryResPressure( 110 )
	BrakeDistributorEmergencyResPressure( 110 )
	BrakeDistributorReleaseRate( 10 )
	BrakeDistributorApplicationRate( 15 )
	BrakeDistributorTrainPipeControlRatio( 2.03 )
	BrakeDistributorNormalFullReleasePressure( 110 )
		Inside (
                	PassengerCabinFile ( BVmot_interior.s )
                	PassengerCabinHeadPos ( -1.03 2.31 0.6 )
                	RotationLimit ( 40 75 40 )
                	StartDirection ( 0 0 0 )
		Sound ( "..\\..\\MAV_Hangok\\gyors\\dzugalt.sms" )
	)
PassengerCapacity ( 60 )
			Lights	(	23
		Light	(
			comment( Sphere of light Mid )
			Type		( 1 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.2 )
			FadeOut	( 0.0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095 )
					Position ( 0.0  1.59 12.75 )
					Transition ( 0 )
					Radius ( 80.0 )
					Angle ( 15.0 )
					)
				)
			)
		Light	(
			comment( Sphere of light Full )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.0 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095 )
					Position ( 0.0  2.09 12.75 )
					Transition ( 0 )
					Radius ( 120.0 )
					Angle ( 20.0 )
					)
				)
			)
comment	( ajtonyitok 8 feny )
		Light	(
			comment( bal oldal eZ )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FF2E8B57 )
					Position 	( 1.42 1.55 6.95 )
					Azimuth 	( 90.0 90.0 90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
	Light	(
			comment( bal oldal hZ )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FF2E8B57 )
					Position 	( 1.36 1.57 -12.62 )
					Azimuth 	( 90.0 90.0 90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
		Light	(
			comment( bal oldal eP )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFff0000 )
					Position 	( 1.42 1.43 6.95 )
					Azimuth 	( 90.0 90.0 90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
		Light	(
			comment( bal oldal hP )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFff0000 )
					Position 	( 1.36 1.45 -12.62 )
					Azimuth 	( 90.0 90.0 90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
		Light	(
			comment( jobb oldal eZ )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FF2E8B57 )
					Position 	( -1.42 1.57 6.95 )
					Azimuth 	( -90.0 -90.0 -90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
		Light	(
			comment( jobb oldal hZ )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FF2E8B57 )
					Position 	( -1.36 1.57 -12.62 )
					Azimuth 	( -90.0 -90.0 -90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
		Light	(
			comment( jobb oldal eP )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFff0000 )
					Position 	( -1.42 1.43 6.95 )
					Azimuth 	( -90.0 -90.0 -90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
		Light	(
			comment( jobb oldal hP )
			Type			( 0 )
			Conditions (
				Headlight 	( 0 )
				Unit 		( 0 )
				TimeOfDay	( 2 )
				)
			FadeIn		( 0.2 )
			FadeOut		( 0.3 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFff0000 )
					Position 	( -1.36 1.45 -12.62 )
					Azimuth 	( -90.0 -90.0 -90.0 )
					Transition 	( 0 )
					Radius 	( 0.1 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
		)
comment (
		comment ( csucsfenyszoro )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095  )
					Position ( 0 3.63 11.75 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				)
			)
)
		comment ( csucsfenyszoro reflektor )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095 )
					Position ( 0 3.63 11.75 )
					Elevation ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				)
			)
		comment ( bal )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095  )
					Position ( -0.67 1.73 12.53 )
					Azimuth 	( -5.0 -5.0 -5.0 )
					Elevation ( 5.0 5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		comment ( bal reflektor )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095 )
					Position ( -0.67 1.73 12.53 )
					Azimuth 	( -5.0 -5.0 -5.0 )
					Elevation ( 5.0 5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.7 )
					)
				)
			)
		comment ( jobb )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095  )
					Position ( 0.67 1.73 12.53 )
					Azimuth 	( 5.0 5.0 5.0 )
					Elevation ( 5.0 5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		comment ( jobb tolatofeny )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 1 )
				Unit ( 2 )
				)
			FadeIn	( 0.0 )
			FadeOut	( 0.0 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 50ff7200  )
					Position ( -0.67 1.73 12.53 )
					Azimuth 	( 0.0 5.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		comment ( jobb tolatofeny REV)
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 1 )
				Unit ( 4 )
				)
			FadeIn	( 0.0 )
			FadeOut	( 0.0 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 50ff7200  )
					Position ( -0.67 1.73  12.53 )
					Azimuth 	( 0.0 5.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)


		comment ( jobb refi )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeffe095 )
					Position ( 0.67 1.73 12.53 )
					Azimuth 	( 5.0 5.0 5.0 )
					Elevation ( 5.0 5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.7 )
					)
				)
			)
		comment ( jobb hatso )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 3 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFff0000  )
					Position ( 0.894 1.634 -12.83 )
					Azimuth ( 180.0 180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		comment ( bal hatso )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 3 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.3 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFff0000  )
					Position ( -0.894 1.634 -12.83 )
					Azimuth ( 180.0 180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
comment ( zarfenyek )
		comment ( bal piros )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.4 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFff0000  )
					Position ( -0.94 1.73 12.51 )
					Transition ( 0 )
					Elevation ( 0 0 0 )
					Azimuth ( 0.0 -5.0 0.0 )
					Radius ( 0.5 )
					)
				)
			)
		comment ( jobb piros )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 4 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.4 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFff0000  )
					Position ( 0.94 1.73 12.51 )
					Transition ( 0 )
					Elevation ( 0 0 0 )
					Azimuth ( 0.0 5.0 0.0 )
					Radius ( 0.5 )
					)
				)
			)
comment ( AI 1feny )
		comment ( AI bal reflektor )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				)
			FadeIn	( 0.0 )
			FadeOut	( 0.0 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 50ff7200 )
					Position ( -0.67 1.73 12.53 )
					Azimuth 	( -5.0 -5.0 -5.0 )
					Elevation ( 5.0 5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		comment ( AI jobb reflektor )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 0 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 0 )
				)
			FadeIn	( 0.0 )
			FadeOut	( 0.0 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 50ff7200 )
					Position ( 0.67 1.73 12.53 )
					Azimuth 	( 5.0 5.0 5.0 )
					Elevation ( 5.0 5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
	)



    	Sound (	BVmot_eng.sms )
)

Engine ( H-Start_90_55_90-76_003-9
	Wagon ( H-Start_90_55_90-76_003-9 )
	Type ( Electric )
	MaxPower ( 1755kW )
        MaxForce ( 180kN )
        MaxContinuousForce ( 202kN )
        MaxVelocity ( 160kph )
        MaxCurrent ( 1700A )
        WheelRadius ( 0.5m )
        Sanding ( 1e1mph )
        NumWheels ( 4 )

  	  CabView ( bvmot.cvf )

#	AirBrakeMaxMainResPipePressure( 145 )
	AirBrakesAirCompressorPowerRating( 1.66 ) comment ( VV450/150 legsurito 2820l/min [6/110]= 1.66 ft3/s )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 145 ) comment ( 10bar = 145psi [6/110] )
	AirBrakesMainResVolume( 42.4 ) comment ( 2x600l = 42.4ft3 [6/189] )
	AirBrakesAirCompressorWattage( 19000 ) comment ( [6/109] )
	AirBrakesCompressorRestartPressure( 128 ) comment ( 8.8bar = 128 psi [6/158] )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.27 ) comment ( Levego igeny fontban. Jelentese nem teljesen vilagos. )
#	AirBrakesHasLowPressureTest( 0 )
	AirBrakesIsCompressorElectricOrMechanical( 1 ) comment ( villamos legsurito )

        EngineBrakesControllerHasProportionalBrake( 0 )
        EngineBrakesProportionalBrakeLag( 0 )

	TrainBrakesControllerMinPressureReduction( 4.35 )
	TrainBrakesControllerMaxApplicationRate( 3.4 ) comment ( 23.2psi/6-8s[4/284]=3.87-2.9psi/s )
	TrainBrakesControllerMaxReleaseRate( 6.18 ) comment ( 23.2psi/3-5s[4/284]=7.73-4.64psi/s )
	TrainBrakesControllerEmergencyApplicationRate( 24 ) comment ( 58psi(5->1bar)/2-3s[4/285]=29-19.3psi/s )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerFullServicePressureDrop( 23.2 )

	DynamicBrakesMinUsableSpeed( 9.3 ) comment ( Villamos fekezes 15km/h(=9.3mph) felett aktiv [6/278][7/104])
	DynamicBrakesMaximumEffectiveSpeed( 1e6 ) comment ( Nincs felso sebesseg hatar )
	DynamicBrakesMaximumForce( 118kN ) comment ( 118kN [6/239][7/131] )
	DynamicBrakesResistorCurrentLimit ( 420A ) comment ( 420A [7/131] )
	DynamicBrakesCutInSpeed( 9.3 ) comment ( Villamos fekezes 15km/h(=9.3mph) felett aktiv [6/278][7/104])
	DynamicBrakesMaxAirBrakePressure ( 1e6 ) comment ( A levegos fekezes nem szunteti meg a villamos fekhatast [7/131] )
	DynamicBrakesFadingSpeed( 17.3 ) comment ( A fekero jelleggorbe alapjan kb 28km/h(=17.3mph) [6/278] )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 ) comment ( kb 2-3s alatt epul fel a fekuzem, de nem MSTS modra )
	DynamicBrakesMaximumSpeedForFadeOut ( 1e6 ) comment ( Nincs felso sebesseg hatar az elektrodinamikus fekezesre )
	DynamicBrakesEffectAtMaximumFadeOut( 1 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 0 ) comment ( Valosagban: To,M,K,1-8,Gy,E {14 db} )

	
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
         	
        BrakesEngineControllers( "Train, Dynamic, Blended" )
	DoesBrakeCutPower( 1 )
	DoesHornTriggerBell( 0 )
	BrakeCutsPowerAtBrakeCylinderPressure( 50 ) comment ( Teljes uzemi fekezeskor a vonoero megszunik )

    	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 0 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 0 )
    		)
		
	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 25 )
		MonitoringDeviceAlarmTimeLimit( 17 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 139 )
		MonitoringDeviceResetLevel( -1 )
		MonitoringDeviceAppliesFullBrake( 0 )
		MonitoringDeviceAppliesEmergencyBrake( 0 )
		MonitoringDeviceAppliesCutsPower( 0 )
		MonitoringDeviceAppliesShutsDownEngine( 0 )
		MonitoringDeviceTriggerOnTrackOverspeed( 0 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 0 )
		MonitoringDeviceResetOnResetButton( 0 )
		)
	
        EngineControllers (
            Throttle ( 0 1 0.05 0 
                NumNotches ( 0 )
            )
            Brake_Train ( 0 1 0.125 0.5 
            NumNotches ( 6
                Notch ( 0       0 TrainBrakesControllerReleaseStart )
                Notch ( 0.2	0 TrainBrakesControllerHoldLappedStart )
                Notch ( 0.25    1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                Notch ( 0.85    0 TrainBrakesControllerSuppressionStart )
                Notch ( 0.9     0 TrainBrakesControllerContinuousServiceStart )
                Notch ( 0.95    0 TrainBrakesControllerEmergencyStart )
            )
        )
            Brake_Dynamic ( 0 1 0.15 0 
                NumNotches ( 0 ) 
	    )

            DirControl ( -1 0 1 1 )
            EmergencyStopToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 ) 
            PantographToggle2 ( 0 1 0 ) 
            PantographsToggle_6 ( 0 1 3 )
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
        )
        Name ( "H-Start BVmot-003" )
        Description (
 	"MAV BVmot "Samu" becenevu motorkocsi"

    )
    EngineOperatingProcedures (
    "To move forward\n"+
    "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
    "2.	Press the W key to move the Reverser to Forward.\n"+
    "3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
    "4.	Press the D key to move increase the throttle setting.\n\n"+  
    "To slow the train\n"+
    "1.	Press the A key to move the throttle to a lower setting.\n"+
    "2.	Use the brakes to further reduce speed if desired.\n\n"+   
    "To apply the train brakes\n"+
    "1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
    "To release the train brakes\n"+
    "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
    "To activate emergency braking\n"+
    "1.	Press the A key to reduce the throttle to Idle.\n"+
    "2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
    "To back up\n"+
    "1.	Bring your train to a full stop.\n"+
    "2.	Press the S key to move the Reverser to the Reverse position.\n"+
    "3.	Press the ; (SEMICOLON)  to release the brakes.\n"+
    "4.	Slowly advance the throttle lever (D key).\n\n"+
    "To load and unload passengers\n"+
    "1. Stop at a station.\n"+
    "2. Press the ENTER key.\n"+
    "3. Wait for the 'permission to depart' signal.\n"+
    "TIP: Use the Next Station driving aid (F10) to monitor loading and unloading."
    ) 
    	Sound (	BVmot_cab.sms )
)
