SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( OBB_4024-067-4
	Type ( Engine )
	WagonShape ( OBB_4024-067-4.s )
	Size ( 2.925m 3.360m 18.40m )
	CentreOfGravity ( 0m 1.7m 0m )
	MaxTilt ( 6.5deg )
	Mass ( 32t )
	WheelRadius ( 0.475m )
	InertiaTensor ( Box (2.9m 3.3m 18.20m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 2e5N/m 0 )
			Damping ( 2e5N/m/s 0 )
			Break ( 3e7N 0 )
			r0 ( 15cm 15cm )
		)
		CouplingHasRigidConnection ( 1 )
	)
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 2e5N/m 0 )
			Damping ( 2e5N/m/s 0 )
			Break ( 3e7N 0 )
			r0 ( 15cm 15cm )
		)
		CouplingHasRigidConnection ( 1 )
	)
	Buffers (
		Spring (
			Stiffness ( 1e8N/m 0N/m )
			Damping ( 1e8N/m/s 0N/m/s)
			r0 ( 0m 1e9 )
		)
		Centre ( 1 )
		Radius ( 2 )
		Angle ( 1deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 7cm )
	DerailRailForce ( 82.24kN )
	DerailBufferForce ( 313.6kN )
	NumWheels ( 3 )					comment ( Räder )
	Friction (
		504.2N/m/s		-0.05		1mph		4.075N/m/s		1.776
		5.1N/rad/s		1		-1rad/s		0		1
	)
	AntiSlip ()

	BrakeEquipmentType( "Air_single_pipe, Distributor, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 51kN )

	EmergencyBrakeResMaxPressure( 72.5 )
	TripleValveRatio( 2.3 )
	MaxReleaseRate( 50 )
	MaxApplicationRate( 9 )
	MaxAuxilaryChargingRate( 4 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 4 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )
	EmergencyResVolumeMultiplier( 1.15 )
	BrakeAirPressureGainInResForOnePoundFromPipe( 0.25 )

	BrakeDistributorFullServicePressure( 50.76 )
	BrakeDistributorMaxAuxilaryResPressure( 72.5 )
	BrakeDistributorEmergencyResPressure( 72.5 )
	BrakeDistributorReleaseRate( 6.59 )
	BrakeDistributorApplicationRate( 9.88 )
	BrakeDistributorTrainPipeControlRatio( 2.03 )
	BrakeDistributorNormalFullReleasePressure( 72.5 )
BrakeDistributorEmergencyApplicationPressure( 50 ) #(nicht dokumentierter Parameter; von CSR aus train.exe extrahiert)
BrakeDistributorEmergencyApplicationRate( 0.25 ) #(nicht dokumentierter Parameter; von CSR aus train.exe extrahiert)

	PassengerCapacity ( 73 )

Sound ( "4024schub.sms" )

	Lights	( 12
		
Light (
comment( Sphere of light Mid )
Type ( 1 )
Conditions (
Headlight ( 2 )
Unit ( 2 )
)
Cycle ( 0 )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State (
Duration ( 0.0 )
LightColour ( eeffe095 )
Position ( 0.0 1 6.4 )
Transition ( 0 )
Radius ( 80.0 )
Angle ( 16.0 )
)
)
)
Light (
comment( Sphere of light Full )
Type ( 1 )
Conditions (
Headlight ( 3 )
Unit ( 2 )
)
Cycle ( 0 )
FadeIn ( 0.5 )
FadeOut ( 0.5 )
States ( 1
State (
Duration ( 0.0 )
LightColour ( eeffe095 )
Position ( 0.0 1.4 18 )
Transition ( 0 )
Radius ( 160.0 )
Angle ( 12.0 )
)
)
)


		Light	(
			comment( bal elso feher DIM+FULL REV )
			Type			( 0 )
			Conditions (
				Headlight 	( 4 )
				Unit 		( 5 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( -0.45 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal elso feher FULL2 REV )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 5 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( -0.69 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb elso feher DIM+FULL REV)
			Type			( 0 )
			Conditions (
				Headlight 	( 4 )
				Unit 		( 5 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( 0.45 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb elso feher FULL2 REV)
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 5 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( 0.69 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal hatso voros FULL )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( ffff0000 )
					Position 	( -0.69 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb hatso voros FULL )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( ffff0000 )
					Position 	( 0.69 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal elso feher FULL1 AI )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( -0.45 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal elso feher FULL2 AI)
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( -0.69 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( jobb elso feher FULL1 AI )
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( 0.45 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.25 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
		Light	(
			comment( bal elso feher FULL2 AI)
			Type			( 0 )
			Conditions (
				Headlight 	( 3 )
				Unit 		( 2 )
Control 	(1)
Service 	(2)
TimeOfDay ( 0 )
				)
			FadeIn		( 0.5 )
			FadeOut		( 0.5 )
			Cycle			( 0 )
			States	( 1
				State	(
					Duration 	( 0.0 )
					LightColour ( FFFFFFFF )
					Position 	( 0.69 2.18 -8.725 )
					Azimuth 	( -180.0 -180.0 -180.0 )
					Transition 	( 0 )
					Radius 	( 0.45 )
					Elevation 	( 0.0 0.0 0.0 )
					)
				)
			)
)
)

Engine ( OBB_4024-067-4
    Wagon ( OBB_4024-067-4 )
    Type ( Electric )
    MaxPower ( 760kW )
    MaxForce ( 53.5kN )
    MaxContinuousForce ( 45kN )
    MaxVelocity ( 140km/h )
    MaxCurrent ( 250A )
    WheelRadius ( 0.475m )
    Sanding ( 1e9mph )
    NumWheels ( 1 )

    CabView ( 4023_b.cvf )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )

	EngineBrakesControllerDirectControlExponent( 2 )

	BrakesEngineControllers( "Train" )
	DoesBrakeCutPower( 1 )
	BrakeCutsPowerAtBrakeCylinderPressure( 25 )				

	AirBrakesAirCompressorPowerRating( 3 )
	AirBrakesMainMinResAirPressure( 72 )
	AirBrakesMainMaxAirPressure( 143 )
	AirBrakesMainResVolume( 10 )
	AirBrakesAirCompressorWattage( 30000 )
	AirBrakesCompressorRestartPressure( 107 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.9 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )
	AirBrakesHasLowPressureTest ( 1 )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxSystemPressure( 72.5 )

	TrainBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMaxApplicationRate( 15 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 40 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72.5 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerFullServicePressureDrop( 28 )
TrainBrakesControllerDirectControlExponent( 1 )

	DynamicBrakesMinUsableSpeed( 1 )
	DynamicBrakesMaximumEffectiveSpeed( 25 )
	DynamicBrakesMaximumForce( 1kn )
	DynamicBrakesResistorCurrentLimit ( 1600 )
	DynamicBrakesCutInSpeed( 1 )
	DynamicBrakesMaxAirBrakePressure ( 150 )
	DynamicBrakesFadingSpeed( 50 )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
	DynamicBrakesMaximumSpeedForFadeOut ( 150 )
	DynamicBrakesEffectAtMaximumFadeOut( 0 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 8 )
	DynamicBrakeHasAutoBailOff( 0 )


	DoesHornTriggerBell( 0 )

	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 38 )
		MonitoringDeviceAlarmTimeLimit ( 30 )
		MonitoringDevicePenaltyTimeLimit ( 5 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 0 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 1 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 2 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		)
	
    EngineControllers (
            Throttle ( 0 1 0.05 0 
                NumNotches ( 11
				    Notch( 0 0 Dummy )
				    Notch( 0.1 0 Dummy )
				    Notch( 0.2 0 Dummy )
				    Notch( 0.3 0 Dummy )
				    Notch( 0.4 0 Dummy )
				    Notch( 0.5 0 Dummy )
				    Notch( 0.6 0 Dummy )
				    Notch( 0.7 0 Dummy )
				    Notch( 0.8 0 Dummy )
				    Notch( 0.9 0 Dummy )
				    Notch( 1 0 Dummy )
                )
            )
            Brake_Train ( 0 1 0.05 0.4
                NumNotches( 4
	    Notch(0    0 TrainBrakesControllerReleaseStart )
	    Notch(0.2  1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart  )
	    Notch(0.9  0 TrainBrakesControllerFullServiceStart )
	    Notch(1.0  0 TrainBrakesControllerEmergencyStart )
                )
            )
            DirControl ( -1 0 1 1 )
            Combined_Control( 0 1 0.5 0.75 throttle train )
            EmergencyStopToggle( 0 1 0 )
            EmergencyStopResetToggle( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BailOffButton( 0 1 0 )
        )

        Name ( "ÖBB 4024 Talent-4" )
        Description (
	"ÖBB 4024 002-7/6024 002-7. \n\n"+
        " \n\n"+
	"Ein Jahr nach der Auslieferung der ersten Einheiten und mehr als ein halbes Jahr nach dem "+
        "ursprünglich vorgesehenen Einsatztermin wurde am "+
        "1. Juli 2004 - nach mehrmaliger Verschiebung "+
        "der Inbetriebnahme endlich mit dem Planeinsatz der Talent-Triebwagen der Reihe 4024 begonnen. "+
        "Derzeit haben nur die Triebwagen 4024.001 bis 008 eine provisorische Einzelzulassung.\n\n"+
        "Sie dürfen kommerziell nur als Sologarnituren und lediglich zwischen Salzburg und Attnang-Puchheim "+
        "beziehungsweise Saalfelden und mit auf 120 km/h verminderter Höchstgeschwindigkeit eingesetzt werden."
       )
	EngineOperatingProcedures (
	""
	)
)
